ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x2605
  Start of program headers:          52 (bytes into file)
  Start of section headers:          1202892 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         4
  Size of section headers:           40 (bytes)
  Number of section headers:         33
  Section header string table index: 32

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 0000c0 000100 00 WAX  0   0  4
  [ 2] text              PROGBITS        00000100 0001c0 006ce8 00  AX  0   0 16
  [ 3] .ARM.exidx        ARM_EXIDX       00006de8 006ea8 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        00006df0 006eb0 000070 00   A  0   0  4
  [ 5] devices           PROGBITS        00006e60 006f20 000090 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        00006ef0 006fb0 000180 00  WA  0   0  4
  [ 7] ctors             PROGBITS        00007070 007130 000008 00  WA  0   0  1
  [ 8] init_array        PROGBITS        00007078 007cdc 000000 00   W  0   0  1
  [ 9] log_const_section PROGBITS        00007078 007138 000040 00   A  0   0  4
  [10] log_backends_sect PROGBITS        000070b8 007178 000020 00   A  0   0  4
  [11] device_handles    PROGBITS        000070d8 007198 000034 00   A  0   0  2
  [12] rodata            PROGBITS        00007110 0071d0 000a00 00   A  0   0 16
  [13] .ramfunc          PROGBITS        20000000 007cdc 000000 00   W  0   0  1
  [14] datas             PROGBITS        20000000 007bd0 0000b0 00  WA  0   0  4
  [15] k_timer_area      PROGBITS        200000b0 007c80 000038 00  WA  0   0  8
  [16] k_mutex_area      PROGBITS        200000e8 007cb8 000014 00  WA  0   0  4
  [17] k_sem_area        PROGBITS        200000fc 007ccc 000010 00  WA  0   0  4
  [18] bss               NOBITS          20000110 007ce0 0009c5 00  WA  0   0  8
  [19] noinit            NOBITS          20000ad8 007ce0 0018e0 00  WA  0   0  8
  [20] .comment          PROGBITS        00000000 007cdc 000079 01  MS  0   0  1
  [21] .debug_aranges    PROGBITS        00000000 007d58 001870 00      0   0  8
  [22] .debug_info       PROGBITS        00000000 0095c8 098962 00      0   0  1
  [23] .debug_abbrev     PROGBITS        00000000 0a1f2a 0106a2 00      0   0  1
  [24] .debug_line       PROGBITS        00000000 0b25cc 02b08a 00      0   0  1
  [25] .debug_frame      PROGBITS        00000000 0dd658 00423c 00      0   0  4
  [26] .debug_str        PROGBITS        00000000 0e1894 00d0fb 01  MS  0   0  1
  [27] .debug_loc        PROGBITS        00000000 0ee98f 021302 00      0   0  1
  [28] .debug_ranges     PROGBITS        00000000 10fc98 007bc0 00      0   0  8
  [29] .ARM.attributes   ARM_ATTRIBUTES  00000000 117858 000031 00      0   0  1
  [30] .symtab           SYMTAB          00000000 11788c 0081e0 10     31 1207  4
  [31] .strtab           STRTAB          00000000 11fa6c 005efe 00      0   0  1
  [32] .shstrtab         STRTAB          00000000 12596a 000162 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x006ea8 0x00006de8 0x00006de8 0x00008 0x00008 R   0x4
  LOAD           0x0000c0 0x00000000 0x00000000 0x07b10 0x07b10 RWE 0x10
  LOAD           0x007bd0 0x20000000 0x00007b10 0x0010c 0x0010c RW  0x8
  LOAD           0x007ce0 0x20000110 0x20000110 0x00000 0x022a8 RW  0x8

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table ctors log_const_sections log_backends_sections device_handles rodata 
   02     datas k_timer_area k_mutex_area k_sem_area 
   03     bss noinit 
