ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x2f65
  Start of program headers:          52 (bytes into file)
  Start of section headers:          1117072 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         5
  Size of section headers:           40 (bytes)
  Number of section headers:         29
  Section header string table index: 28

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 0000e0 000144 00 WAX  0   0  4
  [ 2] text              PROGBITS        00000144 000224 008530 00  AX  0   0  4
  [ 3] .ARM.exidx        ARM_EXIDX       00008674 008754 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        0000867c 00875c 000050 00   A  0   0  4
  [ 5] devices           PROGBITS        000086cc 0087ac 000078 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        00008744 008824 000208 00  WA  0   0  4
  [ 7] device_handles    PROGBITS        0000894c 008a2c 00001e 00   A  0   0  2
  [ 8] log_const_se[...] PROGBITS        0000896c 008a4c 000048 00   A  0   0  4
  [ 9] rodata            PROGBITS        000089c0 008aa0 0012bc 00   A  0   0 16
  [10] .ramfunc          PROGBITS        2000c4e8 009eba 000000 00   W  0   0  1
  [11] datas             PROGBITS        2000c4e8 009d5c 000150 00  WA  0   0  4
  [12] device_states     PROGBITS        2000c638 009eac 00000a 00  WA  0   0  1
  [13] bss               NOBITS          2000c648 009ec0 003c12 00  WA  0   0  8
  [14] noinit            NOBITS          20010260 009ec0 003000 00  WA  0   0  8
  [15] .comment          PROGBITS        00000000 009eba 000040 01  MS  0   0  1
  [16] .debug_aranges    PROGBITS        00000000 009f00 001dd8 00      0   0  8
  [17] .debug_info       PROGBITS        00000000 00bcd8 07bd35 00      0   0  1
  [18] .debug_abbrev     PROGBITS        00000000 087a0d 00f2e7 00      0   0  1
  [19] .debug_line       PROGBITS        00000000 096cf4 0249c1 00      0   0  1
  [20] .debug_frame      PROGBITS        00000000 0bb6b8 004a0c 00      0   0  4
  [21] .debug_str        PROGBITS        00000000 0c00c4 00dec5 01  MS  0   0  1
  [22] .debug_loc        PROGBITS        00000000 0cdf89 02d25f 00      0   0  1
  [23] .debug_ranges     PROGBITS        00000000 0fb1e8 005a38 00      0   0  8
  [24] .ARM.attributes   ARM_ATTRIBUTES  00000000 100c20 000034 00      0   0  1
  [25] .last_section     PROGBITS        00009dd6 009eb6 000004 00   A  0   0  1
  [26] .symtab           SYMTAB          00000000 100c54 0087a0 10     27 1171  4
  [27] .strtab           STRTAB          00000000 1093f4 007667 00      0   0  1
  [28] .shstrtab         STRTAB          00000000 110a5b 000132 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x008754 0x00008674 0x00008674 0x00008 0x00008 R   0x4
  LOAD           0x0000e0 0x00000000 0x00000000 0x09c7c 0x09c7c RWE 0x10
  LOAD           0x009d5c 0x2000c4e8 0x00009c7c 0x0015a 0x0015a RW  0x4
  LOAD           0x009eb6 0x00009dd6 0x00009dd6 0x00004 0x00004 R   0x1
  LOAD           0x000000 0x2000c648 0x2000c648 0x00000 0x06c18 RW  0x8

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table device_handles log_const_sections rodata 
   02     datas device_states 
   03     .last_section 
   04     bss noinit 
