ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x232e5
  Start of program headers:          52 (bytes into file)
  Start of section headers:          4239744 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         4
  Size of section headers:           40 (bytes)
  Number of section headers:         39
  Section header string table index: 38

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        0000c200 0000c0 0000dc 00 WAX  0   0  4
  [ 2] text              PROGBITS        0000c2e0 0001a0 02da70 00  AX  0   0  8
  [ 3] .ARM.exidx        ARM_EXIDX       00039d50 02dc10 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        00039d58 02dc18 000080 00   A  0   0  4
  [ 5] devices           PROGBITS        00039dd8 02dc98 000078 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        00039e50 02dd10 000138 00  WA  0   0  4
  [ 7] bt_l2cap_fix[...] PROGBITS        00039f88 02de48 000024 00   A  0   0  4
  [ 8] bt_conn_cb_area   PROGBITS        00039fac 02de6c 000024 00   A  0   0  4
  [ 9] bt_gatt_serv[...] PROGBITS        00039fd0 02de90 000018 00   A  0   0  4
  [10] settings_han[...] PROGBITS        00039fe8 02dea8 000078 00   A  0   0  4
  [11] log_const_se[...] PROGBITS        0003a060 02df20 000138 00   A  0   0  4
  [12] device_handles    PROGBITS        0003a198 02e058 00001e 00   A  0   0  2
  [13] rodata            PROGBITS        0003a1c0 02e080 004d94 00   A  0   0 16
  [14] .ramfunc          PROGBITS        20000000 033c80 000000 00   W  0   0  1
  [15] datas             PROGBITS        20000000 032e18 000b6d 00  WA  0   0  8
  [16] device_states     PROGBITS        20000b70 033988 000014 00  WA  0   0  4
  [17] k_timer_area      PROGBITS        20000b88 0339a0 000038 00  WA  0   0  8
  [18] k_mem_slab_area   PROGBITS        20000bc0 0339d8 000080 00  WA  0   0  4
  [19] k_mutex_area      PROGBITS        20000c40 033a58 00003c 00  WA  0   0  4
  [20] k_msgq_area       PROGBITS        20000c7c 033a94 000034 00  WA  0   0  4
  [21] k_sem_area        PROGBITS        20000cb0 033ac8 000030 00  WA  0   0  4
  [22] k_queue_area      PROGBITS        20000ce0 033af8 00001c 00  WA  0   0  4
  [23] _net_buf_poo[...] PROGBITS        20000cfc 033b14 00016c 00  WA  0   0  4
  [24] bss               NOBITS          20000e68 033c88 0036d0 00  WA  0   0  8
  [25] noinit            NOBITS          20004540 033c88 00b760 00  WA  0   0 32
  [26] .comment          PROGBITS        00000000 033c80 03596d 00      0   0  1
  [27] .debug_aranges    PROGBITS        00000000 0695f0 0044b8 00      0   0  8
  [28] .debug_info       PROGBITS        00000000 06daa8 23a7c2 00      0   0  1
  [29] .debug_abbrev     PROGBITS        00000000 2a826a 01fc54 00      0   0  1
  [30] .debug_line       PROGBITS        00000000 2c7ebe 05e2e4 00      0   0  1
  [31] .debug_frame      PROGBITS        00000000 3261a4 00cd18 00      0   0  4
  [32] .debug_str        PROGBITS        00000000 332ebc 01ff78 01  MS  0   0  1
  [33] .debug_loc        PROGBITS        00000000 352e34 06f7a9 00      0   0  1
  [34] .debug_ranges     PROGBITS        00000000 3c25e0 014a58 00      0   0  8
  [35] .ARM.attributes   ARM_ATTRIBUTES  00000000 3d7038 000035 00      0   0  1
  [36] .symtab           SYMTAB          00000000 3d7070 020a70 10     37 6071  4
  [37] .strtab           STRTAB          00000000 3f7ae0 0134b7 00      0   0  1
  [38] .shstrtab         STRTAB          00000000 40af97 0001e7 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x02dc10 0x00039d50 0x00039d50 0x00008 0x00008 R   0x4
  LOAD           0x0000c0 0x0000c200 0x0000c200 0x32d54 0x32d54 RWE 0x10
  LOAD           0x032e18 0x20000000 0x0003ef54 0x00e68 0x00e68 RW  0x8
  LOAD           0x000000 0x20000e68 0x20000e68 0x00000 0x0ee38 RW  0x20

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table bt_l2cap_fixed_chan_area bt_conn_cb_area bt_gatt_service_static_area settings_handler_static_area log_const_sections device_handles rodata 
   02     datas device_states k_timer_area k_mem_slab_area k_mutex_area k_msgq_area k_sem_area k_queue_area _net_buf_pool_area 
   03     bss noinit 
