<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="QFN48">
</package>
</packages>
<symbols>
<symbol name="NRF52832">
<pin name="DEC1"/>
<pin name="P0/XL1"/>
<pin name="P1/XL2"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9/NFC1"/>
<pin name="P10/NFC2"/>
<pin name="VDD3"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21/RESET"/>
<pin name="CLK"/>
<pin name="DIO"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="P24"/>
<pin name="ANT"/>
<pin name="VSS2"/>
<pin name="DEC2"/>
<pin name="DEC3"/>
<pin name="XC1"/>
<pin name="XC2"/>
<pin name="VDD2"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="NC"/>
<pin name="VSS"/>
<pin name="DEC4"/>
<pin name="DCC"/>
<pin name="VDD"/>
<pin name="DIE_PAD"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="NRF52832">
<description>Bluetooth 4.0 Low Energy/2.4Ghz
NORDIC SEMICONDUCTOR</description>
<gates>
<gate name="G$1" symbol="NRF52832"/>
</gates>
<devices>
<device name="NRF52832-QFAA" package="QFN48">
<connects>
<connect gate="G$1" pin="ANT" pad="30"/>
<connect gate="G$1" pin="CLK" pad="25"/>
<connect gate="G$1" pin="DCC" pad="47"/>
<connect gate="G$1" pin="DEC1" pad="1"/>
<connect gate="G$1" pin="DEC2" pad="32"/>
<connect gate="G$1" pin="DEC3" pad="33"/>
<connect gate="G$1" pin="DEC4" pad="46"/>
<connect gate="G$1" pin="DIE_PAD" pad="GND"/>
<connect gate="G$1" pin="DIO" pad="26"/>
<connect gate="G$1" pin="NC" pad="44"/>
<connect gate="G$1" pin="P0/XL1" pad="2"/>
<connect gate="G$1" pin="P1/XL2" pad="3"/>
<connect gate="G$1" pin="P10/NFC2" pad="12"/>
<connect gate="G$1" pin="P11" pad="14"/>
<connect gate="G$1" pin="P12" pad="15"/>
<connect gate="G$1" pin="P13" pad="16"/>
<connect gate="G$1" pin="P14" pad="17"/>
<connect gate="G$1" pin="P15" pad="18"/>
<connect gate="G$1" pin="P16" pad="19"/>
<connect gate="G$1" pin="P17" pad="20"/>
<connect gate="G$1" pin="P18" pad="21"/>
<connect gate="G$1" pin="P19" pad="22"/>
<connect gate="G$1" pin="P2" pad="4"/>
<connect gate="G$1" pin="P20" pad="23"/>
<connect gate="G$1" pin="P21/RESET" pad="24"/>
<connect gate="G$1" pin="P22" pad="27"/>
<connect gate="G$1" pin="P23" pad="28"/>
<connect gate="G$1" pin="P24" pad="29"/>
<connect gate="G$1" pin="P25" pad="37"/>
<connect gate="G$1" pin="P26" pad="38"/>
<connect gate="G$1" pin="P27" pad="39"/>
<connect gate="G$1" pin="P28" pad="40"/>
<connect gate="G$1" pin="P29" pad="41"/>
<connect gate="G$1" pin="P3" pad="5"/>
<connect gate="G$1" pin="P30" pad="42"/>
<connect gate="G$1" pin="P31" pad="43"/>
<connect gate="G$1" pin="P4" pad="6"/>
<connect gate="G$1" pin="P5" pad="7"/>
<connect gate="G$1" pin="P6" pad="8"/>
<connect gate="G$1" pin="P7" pad="9"/>
<connect gate="G$1" pin="P8" pad="10"/>
<connect gate="G$1" pin="P9/NFC1" pad="11"/>
<connect gate="G$1" pin="VDD" pad="48"/>
<connect gate="G$1" pin="VDD2" pad="36"/>
<connect gate="G$1" pin="VDD3" pad="13"/>
<connect gate="G$1" pin="VSS" pad="45"/>
<connect gate="G$1" pin="VSS2" pad="31"/>
<connect gate="G$1" pin="XC1" pad="34"/>
<connect gate="G$1" pin="XC2" pad="35"/>
</connects>
<technologies>
<technology name="">
<attribute name="NRF52832" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
