nRF Master Control Panel, 2016-07-15

RelayNordic (E2:07:02:99:99:70)

V 14:52:44.088 Connecting to E2:07:02:99:99:70...

D 14:52:44.089 gatt = device.connectGatt(autoConnect = false)

D 14:52:44.491 [Callback] Connection state changed with status: 0 and new state: CONNECTED (2)

I 14:52:44.493 Connected to E2:07:02:99:99:70

D 14:52:44.496 wait(600ms)

D 14:52:44.505 [Broadcast] Action received: android.bluetooth.device.action.ACL\_CONNECTED

V 14:52:45.114 Discovering services...

D 14:52:45.116 gatt.discoverServices()

D 14:52:47.029 [Callback] Services discovered with status: 0

I 14:52:47.032 Services discovered

V 14:52:47.053 Generic Access (0x1800)

- Device Name [R W] (0x2A00)

- Appearance [R] (0x2A01)

- Peripheral Preferred Connection Parameters [R] (0x2A04)

Generic Attribute (0x1801)

- Service Changed [I] (0x2A05)

   Client Characteristic Configuration (0x2902)

Heart Rate (0x180D)

- Heart Rate Measurement [N] (0x2A37)

   Client Characteristic Configuration (0x2902)

- Body Sensor Location [R] (0x2A38)

Running Speed and Cadence (0x1814)

- RSC Measurement [N] (0x2A53)

   Client Characteristic Configuration (0x2902)

- RSC Feature [R] (0x2A54)

Device Firmware Update Service (00001530-1212-efde-1523-785feabcd123)

- DFU Packet [WNR] (00001532-1212-efde-1523-785feabcd123)

- DFU Control Point [N W] (00001531-1212-efde-1523-785feabcd123)

   Client Characteristic Configuration (0x2902)

- DFU Version [R] (00001534-1212-efde-1523-785feabcd123)

V 14:53:27.874 Disconnecting...

D 14:53:27.878 gatt.disconnect()

D 14:53:27.892 [Callback] Connection state changed with status: 0 and new state: DISCONNECTED (0)

I 14:53:27.899 Disconnected

D 14:53:27.902 gatt.refresh()

D 14:53:27.904 gatt.close()

D 14:53:27.976 [Broadcast] Action received: android.bluetooth.device.action.ACL\_DISCONNECTED

V 14:53:27.978 [DFU] DFU service started

V 14:53:27.980 [DFU] Opening file...

I 14:53:28.039 [DFU] Image file opened (22516 bytes in total)

D 14:53:28.040 [DFU] wait(1000)

V 14:53:29.054 [DFU] Connecting to DFU target...

D 14:53:29.166 [DFU] gatt = device.connectGatt(autoConnect = false)

D 14:53:29.537 [Broadcast] Action received: android.bluetooth.device.action.ACL\_CONNECTED

I 14:53:29.551 [DFU] Connected to E2:07:02:99:99:70

V 14:53:29.552 [DFU] Discovering services...

D 14:53:29.553 [DFU] gatt.discoverServices()

I 14:53:32.000 [DFU] Services discovered

D 14:53:32.006 [DFU] wait(1000)

V 14:53:33.037 [DFU] Reading DFU version number...

I 14:53:33.157 [DFU] Read Response received from 00001534-1212-efde-1523-785feabcd123, value (0x): 01-00

A 14:53:33.159 [DFU] Version number read: 0.1

W 14:53:33.160 [DFU] Application with buttonless update found

V 14:53:33.161 [DFU] Jumping to the DFU Bootloader...

V 14:53:33.163 [DFU] Enabling notifications for 00001531-1212-efde-1523-785feabcd123

D 14:53:33.164 [DFU] gatt.setCharacteristicNotification(00001531-1212-efde-1523-785feabcd123, true)

D 14:53:33.165 [DFU] gatt.writeDescriptor(00002902-0000-1000-8000-00805f9b34fb, value=0x01-00)

V 14:53:33.244 [DFU] Notifications enabled for 00001531-1212-efde-1523-785feabcd123

A 14:53:33.246 [DFU] Notifications enabled

D 14:53:33.247 [DFU] wait(1000)

V 14:53:34.292 [DFU] Writing to characteristic 00001531-1212-efde-1523-785feabcd123

D 14:53:34.294 [DFU] gatt.writeCharacteristic(00001531-1212-efde-1523-785feabcd123)

I 14:53:34.410 [DFU] Data written to 00001531-1212-efde-1523-785feabcd123, value (0x): 01-04

A 14:53:34.411 [DFU] Jump to bootloader sent (Op Code = 1, Upload Mode = 4)

I 14:53:34.483 [DFU] Disconnected by the remote device

D 14:53:34.485 [DFU] gatt.refresh() (hidden)

D 14:53:34.486 [DFU] gatt.close()

D 14:53:34.487 [Broadcast] Action received: android.bluetooth.device.action.ACL\_DISCONNECTED

V 14:53:34.493 [DFU] DFU service started

V 14:53:34.494 [DFU] Opening file...

I 14:53:34.509 [DFU] Image file opened (22516 bytes in total)

D 14:53:34.511 [DFU] wait(1000)

V 14:53:35.525 [DFU] Connecting to DFU target...

D 14:53:35.586 [DFU] gatt = device.connectGatt(autoConnect = false)

D 14:53:36.337 [Broadcast] Action received: android.bluetooth.device.action.ACL\_CONNECTED

I 14:53:36.340 [DFU] Connected to E2:07:02:99:99:70

V 14:53:36.342 [DFU] Discovering services...

D 14:53:36.345 [DFU] gatt.discoverServices()

I 14:53:38.914 [DFU] Services discovered

D 14:53:38.916 [DFU] wait(1000)

V 14:53:39.944 [DFU] Reading DFU version number...

I 14:53:40.042 [DFU] Read Response received from 00001534-1212-efde-1523-785feabcd123, value (0x): 01-00

A 14:53:40.044 [DFU] Version number read: 0.1

W 14:53:40.046 [DFU] Application with buttonless update found

V 14:53:40.048 [DFU] Jumping to the DFU Bootloader...

V 14:53:40.049 [DFU] Enabling notifications for 00001531-1212-efde-1523-785feabcd123

D 14:53:40.051 [DFU] gatt.setCharacteristicNotification(00001531-1212-efde-1523-785feabcd123, true)

D 14:53:40.052 [DFU] gatt.writeDescriptor(00002902-0000-1000-8000-00805f9b34fb, value=0x01-00)

V 14:53:40.196 [DFU] Notifications enabled for 00001531-1212-efde-1523-785feabcd123

A 14:53:40.199 [DFU] Notifications enabled

D 14:53:40.200 [DFU] wait(1000)

V 14:53:41.225 [DFU] Writing to characteristic 00001531-1212-efde-1523-785feabcd123

D 14:53:41.228 [DFU] gatt.writeCharacteristic(00001531-1212-efde-1523-785feabcd123)

I 14:53:41.290 [DFU] Data written to 00001531-1212-efde-1523-785feabcd123, value (0x): 01-04

A 14:53:41.292 [DFU] Jump to bootloader sent (Op Code = 1, Upload Mode = 4)

I 14:53:41.392 [DFU] Disconnected by the remote device

D 14:53:41.394 [DFU] gatt.refresh() (hidden)

D 14:53:41.395 [DFU] gatt.close()

D 14:53:41.397 [Broadcast] Action received: android.bluetooth.device.action.ACL\_DISCONNECTED

V 14:53:41.409 [DFU] DFU service started

V 14:53:41.411 [DFU] Opening file...

I 14:53:41.412 [DFU] Image file opened (22516 bytes in total)

D 14:53:41.413 [DFU] wait(1000)

V 14:53:42.424 [DFU] Connecting to DFU target...

D 14:53:42.425 [DFU] gatt = device.connectGatt(autoConnect = false)

I 14:53:42.606 [DFU] Connected to E2:07:02:99:99:70

V 14:53:42.607 [DFU] Discovering services...

D 14:53:42.608 [DFU] gatt.discoverServices()

D 14:53:42.609 [Broadcast] Action received: android.bluetooth.device.action.ACL\_CONNECTED

I 14:53:45.188 [DFU] Services discovered

D 14:53:45.189 [DFU] wait(1000)

V 14:53:46.206 [DFU] Reading DFU version number...

I 14:53:46.319 [DFU] Read Response received from 00001534-1212-efde-1523-785feabcd123, value (0x): 01-00

A 14:53:46.320 [DFU] Version number read: 0.1

W 14:53:46.321 [DFU] Application with buttonless update found

V 14:53:46.322 [DFU] Jumping to the DFU Bootloader...

V 14:53:46.323 [DFU] Enabling notifications for 00001531-1212-efde-1523-785feabcd123

D 14:53:46.324 [DFU] gatt.setCharacteristicNotification(00001531-1212-efde-1523-785feabcd123, true)

D 14:53:46.325 [DFU] gatt.writeDescriptor(00002902-0000-1000-8000-00805f9b34fb, value=0x01-00)

V 14:53:46.418 [DFU] Notifications enabled for 00001531-1212-efde-1523-785feabcd123

A 14:53:46.420 [DFU] Notifications enabled

D 14:53:46.421 [DFU] wait(1000)

V 14:53:47.421 [DFU] Writing to characteristic 00001531-1212-efde-1523-785feabcd123

D 14:53:47.423 [DFU] gatt.writeCharacteristic(00001531-1212-efde-1523-785feabcd123)

I 14:53:47.532 [DFU] Data written to 00001531-1212-efde-1523-785feabcd123, value (0x): 01-04

A 14:53:47.533 [DFU] Jump to bootloader sent (Op Code = 1, Upload Mode = 4)

I 14:53:47.634 [DFU] Disconnected by the remote device

D 14:53:47.636 [DFU] gatt.refresh() (hidden)

D 14:53:47.637 [DFU] gatt.close()

D 14:53:47.639 [Broadcast] Action received: android.bluetooth.device.action.ACL\_DISCONNECTED

V 14:53:47.651 [DFU] DFU service started

V 14:53:47.652 [DFU] Opening file...

I 14:53:47.667 [DFU] Image file opened (22516 bytes in total)

D 14:53:47.670 [DFU] wait(1000)

V 14:53:48.671 [DFU] Connecting to DFU target...

D 14:53:48.690 [DFU] gatt = device.connectGatt(autoConnect = false)

D 14:53:49.086 [Broadcast] Action received: android.bluetooth.device.action.ACL\_CONNECTED

I 14:53:49.100 [DFU] Connected to E2:07:02:99:99:70

V 14:53:49.101 [DFU] Discovering services...

D 14:53:49.102 [DFU] gatt.discoverServices()

W 14:53:50.602 [DFU] Upload aborted

V 14:53:50.606 [DFU] Disconnecting...

D 14:53:50.607 [DFU] gatt.disconnect()

I 14:53:50.625 [DFU] Disconnected

D 14:53:50.627 [DFU] gatt.refresh() (hidden)

D 14:53:50.628 [DFU] gatt.close()

V 14:53:50.631 Connecting to E2:07:02:99:99:70...

D 14:53:50.635 gatt = device.connectGatt(autoConnect = false)

D 14:53:50.659 [Broadcast] Action received: android.bluetooth.device.action.ACL\_DISCONNECTED

D 14:53:50.664 gatt.close()