# How to modify the S110 based DFU to work with the S310

1. Include the S310 SoftDevice header files instead of the S110 headers:

2. Set the CODE\_REGION\_1\_START define in dfu\_types.h to 0x20000:

3. Change the RAM allocation in the Keil settings to 0x20002400/0x1C00:
