

# How to modify the S110 based DFU to work with the S310

1. Include the S310 SoftDevice header files instead of the S110 headers:  
   
2. Set the CODE\_REGION\_1\_START define in dfu\_types.h to 0x20000:  
   
3. Change the RAM allocation in the Keil settings to 0x20002400/0x1C00:  
   