ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x1ba9
  Start of program headers:          52 (bytes into file)
  Start of section headers:          1024848 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         4
  Size of section headers:           40 (bytes)
  Number of section headers:         29
  Section header string table index: 28

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 0000c0 000100 00 WAX  0   0  4
  [ 2] text              PROGBITS        00000100 0001c0 0056dc 00  AX  0   0  4
  [ 3] .ARM.exidx        ARM_EXIDX       000057dc 00589c 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        000057e4 0058a4 000060 00   A  0   0  4
  [ 5] devices           PROGBITS        00005844 005904 000090 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        000058d4 005994 000180 00  WA  0   0  4
  [ 7] ctors             PROGBITS        00005a54 005b14 000008 00  WA  0   0  1
  [ 8] init_array        PROGBITS        00005a5c 005f10 000000 00   W  0   0  1
  [ 9] device_handles    PROGBITS        00005a5c 005b1c 000034 00   A  0   0  2
  [10] rodata            PROGBITS        00005a90 005b50 0002dc 00   A  0   0 16
  [11] .ramfunc          PROGBITS        20000000 005f10 000000 00   W  0   0  1
  [12] datas             PROGBITS        20000000 005e30 0000a8 00  WA  0   0  4
  [13] k_timer_area      PROGBITS        200000a8 005ed8 000038 00  WA  0   0  8
  [14] bss               NOBITS          200000e0 005f10 000874 00  WA  0   0  8
  [15] noinit            NOBITS          20000958 005f10 001140 00  WA  0   0  8
  [16] .comment          PROGBITS        00000000 005f10 000079 01  MS  0   0  1
  [17] .debug_aranges    PROGBITS        00000000 005f90 001740 00      0   0  8
  [18] .debug_info       PROGBITS        00000000 0076d0 085a0c 00      0   0  1
  [19] .debug_abbrev     PROGBITS        00000000 08d0dc 00d977 00      0   0  1
  [20] .debug_line       PROGBITS        00000000 09aa53 025361 00      0   0  1
  [21] .debug_frame      PROGBITS        00000000 0bfdb4 003978 00      0   0  4
  [22] .debug_str        PROGBITS        00000000 0c372c 00bbd2 01  MS  0   0  1
  [23] .debug_loc        PROGBITS        00000000 0cf2fe 01b6ce 00      0   0  1
  [24] .debug_ranges     PROGBITS        00000000 0ea9d0 003a98 00      0   0  8
  [25] .ARM.attributes   ARM_ATTRIBUTES  00000000 0ee468 000031 00      0   0  1
  [26] .symtab           SYMTAB          00000000 0ee49c 006c80 10     27 1022  4
  [27] .strtab           STRTAB          00000000 0f511c 005113 00      0   0  1
  [28] .shstrtab         STRTAB          00000000 0fa22f 000121 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x00589c 0x000057dc 0x000057dc 0x00008 0x00008 R   0x4
  LOAD           0x0000c0 0x00000000 0x00000000 0x05d6c 0x05d6c RWE 0x10
  LOAD           0x005e30 0x20000000 0x00005d6c 0x000e0 0x000e0 RW  0x8
  LOAD           0x005f10 0x200000e0 0x200000e0 0x00000 0x019b8 RW  0x8

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table ctors device_handles rodata 
   02     datas k_timer_area 
   03     bss noinit 
