ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x2b6d
  Start of program headers:          52 (bytes into file)
  Start of section headers:          1390504 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         4
  Size of section headers:           40 (bytes)
  Number of section headers:         35
  Section header string table index: 34

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 0000c0 000100 00 WAX  0   0  4
  [ 2] text              PROGBITS        00000100 0001c0 007fec 00  AX  0   0  4
  [ 3] .ARM.exidx        ARM_EXIDX       000080ec 0081ac 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        000080f4 0081b4 000078 00   A  0   0  4
  [ 5] devices           PROGBITS        0000816c 00822c 0000a8 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        00008214 0082d4 000180 00  WA  0   0  4
  [ 7] ctors             PROGBITS        00008394 008454 000008 00  WA  0   0  1
  [ 8] init_array        PROGBITS        0000839c 00913c 000000 00   W  0   0  1
  [ 9] log_const_section PROGBITS        0000839c 00845c 000058 00   A  0   0  4
  [10] log_backends_sect PROGBITS        000083f4 0084b4 000020 00   A  0   0  4
  [11] zephyr_dbg_info   PROGBITS        00008414 0084d4 00003c 00  WA  0   0  4
  [12] device_handles    PROGBITS        00008450 008510 000030 00   A  0   0  2
  [13] rodata            PROGBITS        00008480 008540 000b28 00   A  0   0 16
  [14] .ramfunc          PROGBITS        20000000 00913c 000000 00   W  0   0  1
  [15] datas             PROGBITS        20000000 009068 00005c 00  WA  0   0  4
  [16] device_states     PROGBITS        2000005c 0090c4 00001c 00  WA  0   0  4
  [17] k_timer_area      PROGBITS        20000078 0090e0 000038 00  WA  0   0  8
  [18] k_mutex_area      PROGBITS        200000b0 009118 000014 00  WA  0   0  4
  [19] k_sem_area        PROGBITS        200000c4 00912c 000010 00  WA  0   0  4
  [20] bss               NOBITS          200000d8 009140 000ab3 00  WA  0   0  8
  [21] noinit            NOBITS          20000b90 009140 0018e0 00  WA  0   0  8
  [22] .comment          PROGBITS        00000000 00913c 000079 01  MS  0   0  1
  [23] .debug_aranges    PROGBITS        00000000 0091b8 001e20 00      0   0  8
  [24] .debug_info       PROGBITS        00000000 00afd8 0b8c23 00      0   0  1
  [25] .debug_abbrev     PROGBITS        00000000 0c3bfb 011ba5 00      0   0  1
  [26] .debug_line       PROGBITS        00000000 0d57a0 03129d 00      0   0  1
  [27] .debug_frame      PROGBITS        00000000 106a40 004a60 00      0   0  4
  [28] .debug_str        PROGBITS        00000000 10b4a0 00e7ba 01  MS  0   0  1
  [29] .debug_loc        PROGBITS        00000000 119c5a 025ad6 00      0   0  1
  [30] .debug_ranges     PROGBITS        00000000 13f730 004ac8 00      0   0  8
  [31] .ARM.attributes   ARM_ATTRIBUTES  00000000 1441f8 000033 00      0   0  1
  [32] .symtab           SYMTAB          00000000 14422c 008e70 10     33 1421  4
  [33] .strtab           STRTAB          00000000 14d09c 00658a 00      0   0  1
  [34] .shstrtab         STRTAB          00000000 153626 000180 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x0081ac 0x000080ec 0x000080ec 0x00008 0x00008 R   0x4
  LOAD           0x0000c0 0x00000000 0x00000000 0x08fa8 0x08fa8 RWE 0x10
  LOAD           0x009068 0x20000000 0x00008fa8 0x000d4 0x000d4 RW  0x8
  LOAD           0x009140 0x200000d8 0x200000d8 0x00000 0x02398 RW  0x8

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table ctors log_const_sections log_backends_sections zephyr_dbg_info device_handles rodata 
   02     datas device_states k_timer_area k_mutex_area k_sem_area 
   03     bss noinit 
