ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x4499
  Start of program headers:          52 (bytes into file)
  Start of section headers:          1981520 (bytes into file)
  Flags:                             0x5000400, Version5 EABI, hard-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         5
  Size of section headers:           40 (bytes)
  Number of section headers:         33
  Section header string table index: 32

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 0000e0 000100 00 WAX  0   0  4
  [ 2] text              PROGBITS        00000100 0001e0 00da7c 00  AX  0   0  8
  [ 3] .ARM.exidx        ARM_EXIDX       0000db7c 00dc5c 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        0000db84 00dc64 000088 00   A  0   0  4
  [ 5] device_area       PROGBITS        0000dc0c 00dcec 000078 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        0000dc84 00dd64 000180 00  WA  0   0  4
  [ 7] log_const_area    PROGBITS        0000de04 00dee4 0000a0 00   A  0   0  4
  [ 8] rodata            PROGBITS        0000deb0 00df90 000ec4 00   A  0   0 16
  [ 9] .ramfunc          PROGBITS        20000000 00f214 000000 00   W  0   0  1
  [10] datas             PROGBITS        20000000 00ee58 000254 00  WA  0   0  8
  [11] device_states     PROGBITS        20000254 00f0ac 00000c 00  WA  0   0  1
  [12] k_mem_slab_area   PROGBITS        20000260 00f0b8 00001c 00  WA  0   0  4
  [13] k_mutex_area      PROGBITS        2000027c 00f0d4 000064 00  WA  0   0  4
  [14] k_queue_area      PROGBITS        200002e0 00f138 000010 00  WA  0   0  4
  [15] usb_descriptor    PROGBITS        200002f0 00f148 0000a3 00  WA  0   0  1
  [16] usb_cfg_data_area PROGBITS        20000394 00f1ec 000024 00  WA  0   0  4
  [17] bss               NOBITS          200003b8 00f238 0038bd 00  WA  0   0  8
  [18] noinit            NOBITS          20003c80 00f238 004a40 00  WA  0   0 128
  [19] .comment          PROGBITS        00000000 00f214 00009f 01  MS  0   0  1
  [20] .debug_aranges    PROGBITS        00000000 00f2b8 002d00 00      0   0  8
  [21] .debug_info       PROGBITS        00000000 011fb8 10b1cd 00      0   0  1
  [22] .debug_abbrev     PROGBITS        00000000 11d185 016766 00      0   0  1
  [23] .debug_line       PROGBITS        00000000 1338eb 036774 00      0   0  1
  [24] .debug_frame      PROGBITS        00000000 16a060 007198 00      0   0  4
  [25] .debug_str        PROGBITS        00000000 1711f8 0154dd 01  MS  0   0  1
  [26] .debug_loc        PROGBITS        00000000 1866d5 03c39d 00      0   0  1
  [27] .debug_ranges     PROGBITS        00000000 1c2a78 009338 00      0   0  8
  [28] .ARM.attributes   ARM_ATTRIBUTES  00000000 1cbdb0 000034 00      0   0  1
  [29] .last_section     PROGBITS        0000f12c 00f210 000004 00   A  0   0  1
  [30] .symtab           SYMTAB          00000000 1cbde4 00d800 10     31 2113  4
  [31] .strtab           STRTAB          00000000 1d95e4 00a4fc 00      0   0  1
  [32] .shstrtab         STRTAB          00000000 1e3ae0 00016e 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x00dc5c 0x0000db7c 0x0000db7c 0x00008 0x00008 R   0x4
  LOAD           0x0000e0 0x00000000 0x00000000 0x0ed74 0x0ed74 RWE 0x10
  LOAD           0x00ee58 0x20000000 0x0000ed74 0x003b8 0x003b8 RW  0x8
  LOAD           0x00f210 0x0000f12c 0x0000f12c 0x00004 0x00004 R   0x1
  LOAD           0x000000 0x200003b8 0x200003b8 0x00000 0x08308 RW  0x80

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel device_area sw_isr_table log_const_area rodata 
   02     datas device_states k_mem_slab_area k_mutex_area k_queue_area usb_descriptor usb_cfg_data_area 
   03     .last_section 
   04     bss noinit 
