ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x10012e1
  Start of program headers:          52 (bytes into file)
  Start of section headers:          693572 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         4
  Size of section headers:           40 (bytes)
  Number of section headers:         27
  Section header string table index: 26

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        01000000 0000c0 00023c 00 WAX  0   0  4
  [ 2] text              PROGBITS        0100023c 0002fc 004728 00  AX  0   0  4
  [ 3] initlevel         PROGBITS        01004964 004a24 000048 00   A  0   0  4
  [ 4] device_area       PROGBITS        010049ac 004a6c 00003c 00   A  0   0  4
  [ 5] sw_isr_table      PROGBITS        010049e8 004aa8 0000f0 00  WA  0   0  4
  [ 6] log_const_area    PROGBITS        01004ad8 004b98 000048 00   A  0   0  4
  [ 7] rodata            PROGBITS        01004b20 004be0 001228 00   A  0   0 16
  [ 8] .ramfunc          PROGBITS        21000000 005e4e 000000 00   W  0   0  1
  [ 9] datas             PROGBITS        21000000 005e08 00003c 00  WA  0   0  4
  [10] device_states     PROGBITS        2100003c 005e44 000006 00  WA  0   0  1
  [11] bss               NOBITS          21000048 005e50 000180 00  WA  0   0  8
  [12] noinit            NOBITS          210001c8 005e50 000c00 00  WA  0   0  8
  [13] .comment          PROGBITS        00000000 005e4e 000040 01  MS  0   0  1
  [14] .debug_aranges    PROGBITS        00000000 005e90 001160 00      0   0  8
  [15] .debug_info       PROGBITS        00000000 006ff0 04daca 00      0   0  1
  [16] .debug_abbrev     PROGBITS        00000000 054aba 00aadb 00      0   0  1
  [17] .debug_line       PROGBITS        00000000 05f595 0172a4 00      0   0  1
  [18] .debug_frame      PROGBITS        00000000 07683c 0026f0 00      0   0  4
  [19] .debug_str        PROGBITS        00000000 078f2c 00a6a9 01  MS  0   0  1
  [20] .debug_loc        PROGBITS        00000000 0835d5 0164a5 00      0   0  1
  [21] .debug_ranges     PROGBITS        00000000 099a80 003668 00      0   0  8
  [22] .ARM.attributes   ARM_ATTRIBUTES  00000000 09d0e8 000038 00      0   0  1
  [23] .last_section     PROGBITS        01005d8a 005e4a 000004 00   A  0   0  1
  [24] .symtab           SYMTAB          00000000 09d120 006180 10     25 715  4
  [25] .strtab           STRTAB          00000000 0a32a0 00618a 00      0   0  1
  [26] .shstrtab         STRTAB          00000000 0a942a 000118 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  LOAD           0x0000c0 0x01000000 0x01000000 0x05d48 0x05d48 RWE 0x10
  LOAD           0x005e08 0x21000000 0x01005d48 0x00042 0x00042 RW  0x4
  LOAD           0x005e4a 0x01005d8a 0x01005d8a 0x00004 0x00004 R   0x1
  LOAD           0x000000 0x21000048 0x21000048 0x00000 0x00d80 RW  0x8

 Section to Segment mapping:
  Segment Sections...
   00     rom_start text initlevel device_area sw_isr_table log_const_area rodata 
   01     datas device_states 
   02     .last_section 
   03     bss noinit 
