ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x14111
  Start of program headers:          52 (bytes into file)
  Start of section headers:          4812296 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         6
  Size of section headers:           40 (bytes)
  Number of section headers:         43
  Section header string table index: 42

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 000100 0000dc 00 WAX  0   0  4
  [ 2] text              PROGBITS        000000e0 0001e0 02db4c 00  AX  0   0  8
  [ 3] .ARM.exidx        ARM_EXIDX       0002dc2c 02dd2c 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        0002dc34 02dd34 0000a8 00   A  0   0  4
  [ 5] device_area       PROGBITS        0002dcdc 02dddc 000078 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        0002dd54 02de54 000138 00  WA  0   0  4
  [ 7] _static_thre[...] PROGBITS        0002de90 02df90 000030 00  WA  0   0  8
  [ 8] bt_l2cap_fix[...] PROGBITS        0002dec0 02dfc0 000024 00   A  0   0  4
  [ 9] bt_conn_cb_area   PROGBITS        0002dee4 02dfe4 000028 00   A  0   0  4
  [10] bt_gatt_serv[...] PROGBITS        0002df0c 02e00c 000018 00   A  0   0  4
  [11] log_const_area    PROGBITS        0002df24 02e024 000118 00   A  0   0  4
  [12] log_backend_area  PROGBITS        0002e03c 02e13c 000010 00   A  0   0  4
  [13] settings_han[...] PROGBITS        0002e04c 02e14c 000078 00   A  0   0  4
  [14] tbss              NOBITS          0002e0c4 02e1c4 000008 00 WAT  0   0  4
  [15] rodata            PROGBITS        0002e0d0 02e1d0 007a34 00   A  0   0 16
  [16] .ramfunc          PROGBITS        20000000 036704 000000 00   W  0   0  1
  [17] datas             PROGBITS        20000000 035c08 000767 00  WA  0   0  8
  [18] device_states     PROGBITS        20000767 03636f 00000c 00  WA  0   0  1
  [19] log_mpsc_pbu[...] PROGBITS        20000774 03637c 000044 00  WA  0   0  4
  [20] log_msg_ptr_area  PROGBITS        200007b8 0363c0 000004 00  WA  0   0  4
  [21] k_mem_slab_area   PROGBITS        200007bc 0363c4 000060 00  WA  0   0  4
  [22] k_heap_area       PROGBITS        2000081c 036424 000018 00  WA  0   0  4
  [23] k_mutex_area      PROGBITS        20000834 03643c 00003c 00  WA  0   0  4
  [24] k_sem_area        PROGBITS        20000870 036478 000060 00  WA  0   0  4
  [25] k_fifo_area       PROGBITS        200008d0 0364d8 000054 00  WA  0   0  4
  [26] net_buf_pool_area PROGBITS        20000924 03652c 0001d4 00  WA  0   0  4
  [27] bss               NOBITS          20000af8 036738 003782 00  WA  0   0  8
  [28] noinit            NOBITS          20004280 036738 00ad12 00  WA  0   0 64
  [29] .comment          PROGBITS        00000000 036704 000042 01  MS  0   0  1
  [30] .debug_aranges    PROGBITS        00000000 036748 004128 00      0   0  8
  [31] .debug_info       PROGBITS        00000000 03a870 2c09b1 00      0   0  1
  [32] .debug_abbrev     PROGBITS        00000000 2fb221 020dfe 00      0   0  1
  [33] .debug_line       PROGBITS        00000000 31c01f 06a7d3 00      0   0  1
  [34] .debug_frame      PROGBITS        00000000 3867f4 00c2cc 00      0   0  4
  [35] .debug_str        PROGBITS        00000000 392ac0 023768 01  MS  0   0  1
  [36] .debug_loc        PROGBITS        00000000 3b6228 094077 00      0   0  1
  [37] .debug_ranges     PROGBITS        00000000 44a2a0 0156e8 00      0   0  8
  [38] .ARM.attributes   ARM_ATTRIBUTES  00000000 45f988 000032 00      0   0  1
  [39] .last_section     PROGBITS        000365fc 036700 000004 00   A  0   0  1
  [40] .symtab           SYMTAB          00000000 45f9bc 01f6e0 10     41 5555  4
  [41] .strtab           STRTAB          00000000 47f09c 017b43 00      0   0  1
  [42] .shstrtab         STRTAB          00000000 496bdf 000226 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x02dd2c 0x0002dc2c 0x0002dc2c 0x00008 0x00008 R   0x4
  LOAD           0x000100 0x00000000 0x00000000 0x35b04 0x35b04 RWE 0x10
  LOAD           0x035c08 0x20000000 0x00035b04 0x00af8 0x00af8 RW  0x8
  LOAD           0x036700 0x000365fc 0x000365fc 0x00004 0x00004 R   0x1
  LOAD           0x000000 0x20000af8 0x20000af8 0x00000 0x0e49a RW  0x40
  TLS            0x02e1c4 0x0002e0c4 0x0002e0c4 0x00000 0x00008 R   0x4

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel device_area sw_isr_table _static_thread_data_area bt_l2cap_fixed_chan_area bt_conn_cb_area bt_gatt_service_static_area log_const_area log_backend_area settings_handler_static_area rodata 
   02     datas device_states log_mpsc_pbuf_area log_msg_ptr_area k_mem_slab_area k_heap_area k_mutex_area k_sem_area k_fifo_area net_buf_pool_area 
   03     .last_section 
   04     bss noinit 
   05     tbss 
