ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x1002111
  Start of program headers:          52 (bytes into file)
  Start of section headers:          628524 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         5
  Size of section headers:           40 (bytes)
  Number of section headers:         29
  Section header string table index: 28

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        01000000 0000e0 00023c 00 WAX  0   0  4
  [ 2] text              PROGBITS        01000240 000320 004468 00  AX  0   0  8
  [ 3] .ARM.exidx        ARM_EXIDX       010046a8 004788 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        010046b0 004790 000038 00   A  0   0  4
  [ 5] devices           PROGBITS        010046e8 0047c8 000048 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        01004730 004810 0000f0 00  WA  0   0  4
  [ 7] device_handles    PROGBITS        01004820 004900 000012 00   A  0   0  2
  [ 8] log_const_se[...] PROGBITS        01004834 004914 000058 00   A  0   0  4
  [ 9] rodata            PROGBITS        01004890 004970 001198 00   A  0   0 16
  [10] .ramfunc          PROGBITS        21000000 005b46 000000 00   W  0   0  1
  [11] datas             PROGBITS        21000000 005b08 000034 00  WA  0   0  4
  [12] device_states     PROGBITS        21000034 005b3c 000006 00  WA  0   0  1
  [13] bss               NOBITS          21000040 005b48 000146 00  WA  0   0  8
  [14] noinit            NOBITS          21000188 005b48 000c00 00  WA  0   0  8
  [15] .comment          PROGBITS        00000000 005b46 000040 01  MS  0   0  1
  [16] .debug_aranges    PROGBITS        00000000 005b88 001038 00      0   0  8
  [17] .debug_info       PROGBITS        00000000 006bc0 048387 00      0   0  1
  [18] .debug_abbrev     PROGBITS        00000000 04ef47 009e14 00      0   0  1
  [19] .debug_line       PROGBITS        00000000 058d5b 01330d 00      0   0  1
  [20] .debug_frame      PROGBITS        00000000 06c068 0022f8 00      0   0  4
  [21] .debug_str        PROGBITS        00000000 06e360 0090dd 01  MS  0   0  1
  [22] .debug_loc        PROGBITS        00000000 07743d 013e2b 00      0   0  1
  [23] .debug_ranges     PROGBITS        00000000 08b268 002f68 00      0   0  8
  [24] .ARM.attributes   ARM_ATTRIBUTES  00000000 08e1d0 000034 00      0   0  1
  [25] .last_section     PROGBITS        01005a62 005b42 000004 00   A  0   0  1
  [26] .symtab           SYMTAB          00000000 08e204 005b30 10     27 666  4
  [27] .strtab           STRTAB          00000000 093d34 0058c3 00      0   0  1
  [28] .shstrtab         STRTAB          00000000 0995f7 000132 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x004788 0x010046a8 0x010046a8 0x00008 0x00008 R   0x4
  LOAD           0x0000e0 0x01000000 0x01000000 0x05a28 0x05a28 RWE 0x10
  LOAD           0x005b08 0x21000000 0x01005a28 0x0003a 0x0003a RW  0x4
  LOAD           0x005b42 0x01005a62 0x01005a62 0x00004 0x00004 R   0x1
  LOAD           0x000000 0x21000040 0x21000040 0x00000 0x00d48 RW  0x8

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table device_handles log_const_sections rodata 
   02     datas device_states 
   03     .last_section 
   04     bss noinit 
