ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x102d549
  Start of program headers:          52 (bytes into file)
  Start of section headers:          1735668 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         5
  Size of section headers:           40 (bytes)
  Number of section headers:         34
  Section header string table index: 33

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        01008800 0000e0 00023c 00 WAX  0   0  4
  [ 2] text              PROGBITS        01008a3c 00031c 02c30c 00  AX  0   0  4
  [ 3] .ARM.exidx        ARM_EXIDX       01034d48 02c628 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        01034d50 02c630 000088 00   A  0   0  4
  [ 5] devices           PROGBITS        01034dd8 02c6b8 0000a8 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        01034e80 02c760 0000f0 00  WA  0   0  4
  [ 7] device_handles    PROGBITS        01034f70 02c850 00002e 00   A  0   0  2
  [ 8] log_const_se[...] PROGBITS        01034fa0 02c880 000098 00   A  0   0  4
  [ 9] rodata            PROGBITS        01035040 02c920 000ca0 00   A  0   0 16
  [10] .ramfunc          PROGBITS        21000000 02dd1c 000000 00   W  0   0  1
  [11] datas             PROGBITS        21000000 02d5c0 000654 00  WA  0   0  8
  [12] device_states     PROGBITS        21000654 02dc14 00000e 00  WA  0   0  1
  [13] k_heap_area       PROGBITS        21000664 02dc24 000014 00  WA  0   0  4
  [14] k_mutex_area      PROGBITS        21000678 02dc38 000014 00  WA  0   0  4
  [15] k_sem_area        PROGBITS        2100068c 02dc4c 000018 00  WA  0   0  4
  [16] k_queue_area      PROGBITS        210006a4 02dc64 000030 00  WA  0   0  4
  [17] _net_buf_poo[...] PROGBITS        210006d4 02dc94 000084 00  WA  0   0  4
  [18] bss               NOBITS          21000758 02dd20 003abe 00  WA  0   0  8
  [19] noinit            NOBITS          21004218 02dd20 00664c 00  WA  0   0  8
  [20] .comment          PROGBITS        00000000 02dd1c 000040 01  MS  0   0  1
  [21] .debug_aranges    PROGBITS        00000000 02dd60 002110 00      0   0  8
  [22] .debug_info       PROGBITS        00000000 02fe70 0b3d19 00      0   0  1
  [23] .debug_abbrev     PROGBITS        00000000 0e3b89 012c45 00      0   0  1
  [24] .debug_line       PROGBITS        00000000 0f67ce 02a061 00      0   0  1
  [25] .debug_frame      PROGBITS        00000000 120830 00509c 00      0   0  4
  [26] .debug_str        PROGBITS        00000000 1258cc 0177a9 01  MS  0   0  1
  [27] .debug_loc        PROGBITS        00000000 13d075 034534 00      0   0  1
  [28] .debug_ranges     PROGBITS        00000000 1715b0 0080d0 00      0   0  8
  [29] .ARM.attributes   ARM_ATTRIBUTES  00000000 179680 000034 00      0   0  1
  [30] .last_section     PROGBITS        01036438 02dd18 000004 00   A  0   0  1
  [31] .symtab           SYMTAB          00000000 1796b4 018bd0 10     32 4309  4
  [32] .strtab           STRTAB          00000000 192284 0157f9 00      0   0  1
  [33] .shstrtab         STRTAB          00000000 1a7a7d 000176 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x02c628 0x01034d48 0x01034d48 0x00008 0x00008 R   0x4
  LOAD           0x0000e0 0x01008800 0x01008800 0x2d4e0 0x2d4e0 RWE 0x10
  LOAD           0x02d5c0 0x21000000 0x01035ce0 0x00758 0x00758 RW  0x8
  LOAD           0x02dd18 0x01036438 0x01036438 0x00004 0x00004 R   0x1
  LOAD           0x000000 0x21000758 0x21000758 0x00000 0x0a10c RW  0x8

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table device_handles log_const_sections rodata 
   02     datas device_states k_heap_area k_mutex_area k_sem_area k_queue_area _net_buf_pool_area 
   03     .last_section 
   04     bss noinit 
