ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x7041
  Start of program headers:          52 (bytes into file)
  Start of section headers:          3856728 (bytes into file)
  Flags:                             0x5000400, Version5 EABI, hard-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         5
  Size of section headers:           40 (bytes)
  Number of section headers:         37
  Section header string table index: 36

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 0000e0 000100 00 WAX  0   0  4
  [ 2] text              PROGBITS        00000100 0001e0 051408 00  AX  0   0  8
  [ 3] .ARM.exidx        ARM_EXIDX       00051508 0515e8 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        00051510 0515f0 0000e0 00   A  0   0  4
  [ 5] devices           PROGBITS        000515f0 0516d0 000138 00   A  0   0  4
  [ 6] device_handles    PROGBITS        00051728 051808 00004e 00   A  0   0  2
  [ 7] log_const_se[...] PROGBITS        00051778 051858 000100 00   A  0   0  4
  [ 8] rodata            PROGBITS        00051880 051960 003558 00   A  0   0 16
  [ 9] .ramfunc          PROGBITS        20000000 0558b0 000000 00   W  0   0  1
  [10] datas             PROGBITS        20000000 054eb8 0006a5 00  WA  0   0  4
  [11] sw_isr_table      PROGBITS        200006a8 055560 000180 00  WA  0   0  4
  [12] device_states     PROGBITS        20000828 0556e0 00001a 00  WA  0   0  1
  [13] k_mem_slab_area   PROGBITS        20000844 0556fc 000040 00  WA  0   0  4
  [14] k_heap_area       PROGBITS        20000884 05573c 000018 00  WA  0   0  4
  [15] k_mutex_area      PROGBITS        2000089c 055754 00008c 00  WA  0   0  4
  [16] k_msgq_area       PROGBITS        20000928 0557e0 000034 00  WA  0   0  4
  [17] _net_buf_poo[...] PROGBITS        2000095c 055814 000068 00  WA  0   0  4
  [18] net_if_area       PROGBITS        200009c4 05587c 000004 00  WA  0   0  4
  [19] net_if_dev_area   PROGBITS        200009c8 055880 00001c 00  WA  0   0  4
  [20] net_l2_area       PROGBITS        200009e4 05589c 000010 00   A  0   0  4
  [21] bss               NOBITS          20000a00 055900 00a438 00  WA  0   0 128
  [22] noinit            NOBITS          2000ae80 055900 005d70 00  WA  0   0 128
  [23] .comment          PROGBITS        00000000 0558b0 0000b9 01  MS  0   0  1
  [24] .debug_aranges    PROGBITS        00000000 055970 005230 00      0   0  8
  [25] .debug_info       PROGBITS        00000000 05aba0 1b5102 00      0   0  1
  [26] .debug_abbrev     PROGBITS        00000000 20fca2 027796 00      0   0  1
  [27] .debug_line       PROGBITS        00000000 237438 069605 00      0   0  1
  [28] .debug_frame      PROGBITS        00000000 2a0a40 00e848 00      0   0  4
  [29] .debug_str        PROGBITS        00000000 2af288 036476 01  MS  0   0  1
  [30] .debug_loc        PROGBITS        00000000 2e56fe 070c1a 00      0   0  1
  [31] .debug_ranges     PROGBITS        00000000 356318 010f30 00      0   0  8
  [32] .ARM.attributes   ARM_ATTRIBUTES  00000000 367248 000036 00      0   0  1
  [33] .last_section     PROGBITS        000557cc 0558ac 000004 00   A  0   0  1
  [34] .symtab           SYMTAB          00000000 367280 02a7c0 10     35 7653  4
  [35] .strtab           STRTAB          00000000 391a40 01bd74 00      0   0  1
  [36] .shstrtab         STRTAB          00000000 3ad7b4 0001a2 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x0515e8 0x00051508 0x00051508 0x00008 0x00008 R   0x4
  LOAD           0x0000e0 0x00000000 0x00000000 0x54dd8 0x54dd8 RWE 0x10
  LOAD           0x054eb8 0x20000000 0x00054dd8 0x009f4 0x009f4 RW  0x4
  LOAD           0x0558ac 0x000557cc 0x000557cc 0x00004 0x00004 R   0x1
  LOAD           0x000000 0x20000a00 0x20000a00 0x00000 0x101f0 RW  0x80

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices device_handles log_const_sections rodata 
   02     datas sw_isr_table device_states k_mem_slab_area k_heap_area k_mutex_area k_msgq_area _net_buf_pool_area net_if_area net_if_dev_area net_l2_area 
   03     .last_section 
   04     bss noinit 
