ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x1031e1d
  Start of program headers:          52 (bytes into file)
  Start of section headers:          1913596 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         6
  Size of section headers:           40 (bytes)
  Number of section headers:         33
  Section header string table index: 32

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        01000000 000100 0000b8 00 WAX  0   0  4
  [ 2] text              PROGBITS        010000b8 0001b8 03ad3c 00  AX  0   0  8
  [ 3] .ARM.exidx        ARM_EXIDX       0103adf4 03aef4 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        0103adfc 03aefc 000090 00   A  0   0  4
  [ 5] device_area       PROGBITS        0103ae8c 03af8c 00008c 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        0103af18 03b018 0000f0 00  WA  0   0  4
  [ 7] tbss              NOBITS          0103b008 03b108 000004 00 WAT  0   0  4
  [ 8] rodata            PROGBITS        0103b010 03b110 000ca8 00   A  0   0 16
  [ 9] .ramfunc          PROGBITS        21000000 03c5f4 000000 00   W  0   0  1
  [10] datas             PROGBITS        21000000 03bdb8 000708 00  WA  0   0  8
  [11] device_states     PROGBITS        21000708 03c4c0 00000e 00  WA  0   0  1
  [12] k_heap_area       PROGBITS        21000718 03c4d0 000014 00  WA  0   0  4
  [13] k_mutex_area      PROGBITS        2100072c 03c4e4 000014 00  WA  0   0  4
  [14] k_sem_area        PROGBITS        21000740 03c4f8 000018 00  WA  0   0  4
  [15] k_fifo_area       PROGBITS        21000758 03c510 000030 00  WA  0   0  4
  [16] net_buf_pool_area PROGBITS        21000788 03c540 0000b0 00  WA  0   0  4
  [17] bss               NOBITS          21000838 03c5f8 007016 00  WA  0   0  8
  [18] noinit            NOBITS          21007850 03c5f8 005860 00  WA  0   0  8
  [19] .comment          PROGBITS        00000000 03c5f4 000040 01  MS  0   0  1
  [20] .debug_aranges    PROGBITS        00000000 03c638 002220 00      0   0  8
  [21] .debug_info       PROGBITS        00000000 03e858 0bdeb7 00      0   0  1
  [22] .debug_abbrev     PROGBITS        00000000 0fc70f 013544 00      0   0  1
  [23] .debug_line       PROGBITS        00000000 10fc53 02e8a0 00      0   0  1
  [24] .debug_frame      PROGBITS        00000000 13e4f4 005364 00      0   0  4
  [25] .debug_str        PROGBITS        00000000 143858 01b1ec 01  MS  0   0  1
  [26] .debug_loc        PROGBITS        00000000 15ea44 033bf3 00      0   0  1
  [27] .debug_ranges     PROGBITS        00000000 192638 0080a0 00      0   0  8
  [28] .ARM.attributes   ARM_ATTRIBUTES  00000000 19a6d8 000038 00      0   0  1
  [29] .last_section     PROGBITS        0103c4f0 03c5f0 000004 00   A  0   0  1
  [30] .symtab           SYMTAB          00000000 19a710 01d710 10     31 5041  4
  [31] .strtab           STRTAB          00000000 1b7e20 01b385 00      0   0  1
  [32] .shstrtab         STRTAB          00000000 1d31a5 000157 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x03aef4 0x0103adf4 0x0103adf4 0x00008 0x00008 R   0x4
  LOAD           0x000100 0x01000000 0x01000000 0x3bcb8 0x3bcb8 RWE 0x10
  LOAD           0x03bdb8 0x21000000 0x0103bcb8 0x00838 0x00838 RW  0x8
  LOAD           0x03c5f0 0x0103c4f0 0x0103c4f0 0x00004 0x00004 R   0x1
  LOAD           0x000000 0x21000838 0x21000838 0x00000 0x0c878 RW  0x8
  TLS            0x03b108 0x0103b008 0x0103b008 0x00000 0x00004 R   0x4

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel device_area sw_isr_table rodata 
   02     datas device_states k_heap_area k_mutex_area k_sem_area k_fifo_area net_buf_pool_area 
   03     .last_section 
   04     bss noinit 
   05     tbss 
