ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x3ed5
  Start of program headers:          52 (bytes into file)
  Start of section headers:          1836952 (bytes into file)
  Flags:                             0x5000400, Version5 EABI, hard-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         5
  Size of section headers:           40 (bytes)
  Number of section headers:         34
  Section header string table index: 33

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 0000e0 000100 00 WAX  0   0  4
  [ 2] text              PROGBITS        00000100 0001e0 00c9ec 00  AX  0   0  8
  [ 3] .ARM.exidx        ARM_EXIDX       0000caec 00cbcc 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        0000caf4 00cbd4 0000a0 00   A  0   0  4
  [ 5] devices           PROGBITS        0000cb94 00cc74 0000a8 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        0000cc3c 00cd1c 000180 00  WA  0   0  4
  [ 7] device_handles    PROGBITS        0000cdbc 00ce9c 00002a 00   A  0   0  2
  [ 8] log_const_se[...] PROGBITS        0000cde8 00cec8 000078 00   A  0   0  4
  [ 9] rodata            PROGBITS        0000ce60 00cf40 001938 00   A  0   0 16
  [10] .ramfunc          PROGBITS        20000000 00ec4c 000000 00   W  0   0  1
  [11] datas             PROGBITS        20000000 00e878 000268 00  WA  0   0  4
  [12] device_states     PROGBITS        20000268 00eae0 00000e 00  WA  0   0  1
  [13] k_mem_slab_area   PROGBITS        20000278 00eaf0 00001c 00  WA  0   0  4
  [14] k_mutex_area      PROGBITS        20000294 00eb0c 000064 00  WA  0   0  4
  [15] k_queue_area      PROGBITS        200002f8 00eb70 000010 00  WA  0   0  4
  [16] usb_descriptor    PROGBITS        20000308 00eb80 0000a3 00  WA  0   0  1
  [17] usb_cfg_data_area PROGBITS        200003ac 00ec24 000024 00  WA  0   0  4
  [18] bss               NOBITS          200003d0 00ec50 002c25 00  WA  0   0  8
  [19] noinit            NOBITS          20003000 00ec50 004a40 00  WA  0   0 128
  [20] .comment          PROGBITS        00000000 00ec4c 0000bf 01  MS  0   0  1
  [21] .debug_aranges    PROGBITS        00000000 00ed10 002928 00      0   0  8
  [22] .debug_info       PROGBITS        00000000 011638 0f4821 00      0   0  1
  [23] .debug_abbrev     PROGBITS        00000000 105e59 01523c 00      0   0  1
  [24] .debug_line       PROGBITS        00000000 11b095 033177 00      0   0  1
  [25] .debug_frame      PROGBITS        00000000 14e20c 006628 00      0   0  4
  [26] .debug_str        PROGBITS        00000000 154834 0141d1 01  MS  0   0  1
  [27] .debug_loc        PROGBITS        00000000 168a05 0385c2 00      0   0  1
  [28] .debug_ranges     PROGBITS        00000000 1a0fc8 009068 00      0   0  8
  [29] .ARM.attributes   ARM_ATTRIBUTES  00000000 1aa030 000034 00      0   0  1
  [30] .last_section     PROGBITS        0000eb68 00ec48 000004 00   A  0   0  1
  [31] .symtab           SYMTAB          00000000 1aa064 00cc70 10     32 2029  4
  [32] .strtab           STRTAB          00000000 1b6cd4 009947 00      0   0  1
  [33] .shstrtab         STRTAB          00000000 1c061b 00017d 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x00cbcc 0x0000caec 0x0000caec 0x00008 0x00008 R   0x4
  LOAD           0x0000e0 0x00000000 0x00000000 0x0e798 0x0e798 RWE 0x10
  LOAD           0x00e878 0x20000000 0x0000e798 0x003d0 0x003d0 RW  0x4
  LOAD           0x00ec48 0x0000eb68 0x0000eb68 0x00004 0x00004 R   0x1
  LOAD           0x000000 0x200003d0 0x200003d0 0x00000 0x07670 RW  0x80

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table device_handles log_const_sections rodata 
   02     datas device_states k_mem_slab_area k_mutex_area k_queue_area usb_descriptor usb_cfg_data_area 
   03     .last_section 
   04     bss noinit 
