ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0xa7d5
  Start of program headers:          52 (bytes into file)
  Start of section headers:          3923488 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         6
  Size of section headers:           40 (bytes)
  Number of section headers:         48
  Section header string table index: 47

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 000100 0004c8 00  AX  0   0  4
  [ 2] text              PROGBITS        000004c8 0005c8 018800 00  AX  0   0  8
  [ 3] .ARM.exidx        ARM_EXIDX       00018cc8 018dc8 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        00018cd0 018dd0 0000b8 00   A  0   0  4
  [ 5] device_area       PROGBITS        00018d88 018e88 000144 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        00018ecc 018fcc 000910 00   A  0   0  4
  [ 7] entropy_driv[...] PROGBITS        000197dc 0198dc 000008 00   A  0   0  4
  [ 8] gpio_driver_[...] PROGBITS        000197e4 0198e4 000024 00   A  0   0  4
  [ 9] clock_contro[...] PROGBITS        00019808 019908 00001c 00   A  0   0  4
  [10] uart_driver_[...] PROGBITS        00019824 019924 000098 00   A  0   0  4
  [11] log_const_area    PROGBITS        000198bc 0199bc 000130 00   A  0   0  4
  [12] log_backend_area  PROGBITS        000199ec 019aec 000010 00   A  0   0  4
  [13] zephyr_dbg_info   PROGBITS        000199fc 019afc 000044 00   A  0   0  4
  [14] tbss              NOBITS          00019a40 019b40 000008 00 WAT  0   0  4
  [15] rodata            PROGBITS        00019a40 019b40 002170 00   A  0   0 16
  [16] NRF_KMU_RESE[...] NOBITS          20000000 01c910 000040 00  WA  0   0  1
  [17] .ramfunc          PROGBITS        20000040 01c90c 000000 00   W  0   0  1
  [18] datas             PROGBITS        20000040 01bcb0 00091f 00  WA  0   0  8
  [19] device_states     PROGBITS        2000095f 01c5cf 000015 00  WA  0   0  1
  [20] log_mpsc_pbu[...] PROGBITS        20000974 01c5e4 000040 00  WA  0   0  4
  [21] log_msg_ptr_area  PROGBITS        200009b4 01c624 000004 00  WA  0   0  4
  [22] k_mem_slab_area   PROGBITS        200009b8 01c628 00001c 00  WA  0   0  4
  [23] k_heap_area       PROGBITS        200009d4 01c644 000014 00  WA  0   0  4
  [24] k_mutex_area      PROGBITS        200009e8 01c658 000078 00  WA  0   0  4
  [25] k_msgq_area       PROGBITS        20000a60 01c6d0 000030 00  WA  0   0  4
  [26] k_sem_area        PROGBITS        20000a90 01c700 000030 00  WA  0   0  4
  [27] k_event_area      PROGBITS        20000ac0 01c730 000024 00  WA  0   0  4
  [28] net_buf_pool_area PROGBITS        20000ae4 01c754 000108 00  WA  0   0  4
  [29] usbd_context_area PROGBITS        20000bec 01c85c 00007c 00  WA  0   0  4
  [30] usbd_class_f[...] PROGBITS        20000c68 01c8d8 000018 00  WA  0   0  4
  [31] usbd_class_h[...] PROGBITS        20000c80 01c8f0 000018 00  WA  0   0  4
  [32] .comment          PROGBITS        00000000 01c90c 000020 01  MS  0   0  1
  [33] .debug_aranges    PROGBITS        00000000 01c930 003d90 00      0   0  8
  [34] .debug_info       PROGBITS        00000000 0206c0 2289a1 00      0   0  1
  [35] .debug_abbrev     PROGBITS        00000000 249061 022a9b 00      0   0  1
  [36] .debug_line       PROGBITS        00000000 26bafc 06accb 00      0   0  1
  [37] .debug_frame      PROGBITS        00000000 2d67c8 00a678 00      0   0  4
  [38] .debug_str        PROGBITS        00000000 2e0e40 026700 01  MS  0   0  1
  [39] .debug_loc        PROGBITS        00000000 307540 0799a2 00      0   0  1
  [40] .debug_ranges     PROGBITS        00000000 380ee8 012e30 00      0   0  8
  [41] .ARM.attributes   ARM_ATTRIBUTES  00000000 393d18 000038 00      0   0  1
  [42] .last_section     PROGBITS        0001c808 01c908 000004 00  WA  0   0  4
  [43] bss               NOBITS          20000c98 01c910 003118 00  WA  0   0  8
  [44] noinit            NOBITS          20003db0 01c910 0041f0 00  WA  0   0  8
  [45] .symtab           SYMTAB          00000000 393d50 0166a0 10     46 3543  4
  [46] .strtab           STRTAB          00000000 3aa3f0 0137b2 00      0   0  1
  [47] .shstrtab         STRTAB          00000000 3bdba2 00027e 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  D (mbind), y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x018dc8 0x00018cc8 0x00018cc8 0x00008 0x00008 R   0x4
  LOAD           0x000100 0x00000000 0x00000000 0x1bbb0 0x1bbb0 RWE 0x10
  LOAD           0x01bcb0 0x20000040 0x0001bbb0 0x00c58 0x00c58 RW  0x8
  LOAD           0x01c908 0x0001c808 0x0001c808 0x00004 0x00004 RW  0x4
  LOAD           0x000000 0x20000000 0x20000000 0x00000 0x07fa0 RW  0x8
  TLS            0x019b40 0x00019a40 0x00019a40 0x00000 0x00008 R   0x4

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel device_area sw_isr_table entropy_driver_api_area gpio_driver_api_area clock_control_driver_api_area uart_driver_api_area log_const_area log_backend_area zephyr_dbg_info rodata 
   02     datas device_states log_mpsc_pbuf_area log_msg_ptr_area k_mem_slab_area k_heap_area k_mutex_area k_msgq_area k_sem_area k_event_area net_buf_pool_area usbd_context_area usbd_class_fs_area usbd_class_hs_area 
   03     .last_section 
   04     NRF_KMU_RESERVED_PUSH_SECTION bss noinit 
   05     tbss 
