ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x230dd
  Start of program headers:          52 (bytes into file)
  Start of section headers:          3966840 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         4
  Size of section headers:           40 (bytes)
  Number of section headers:         39
  Section header string table index: 38

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        0000c200 0000c0 0000dc 00 WAX  0   0  4
  [ 2] text              PROGBITS        0000c2e0 0001a0 02e510 00  AX  0   0  8
  [ 3] .ARM.exidx        ARM_EXIDX       0003a7f0 02e6b0 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        0003a7f8 02e6b8 000080 00   A  0   0  4
  [ 5] devices           PROGBITS        0003a878 02e738 000078 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        0003a8f0 02e7b0 000138 00  WA  0   0  4
  [ 7] bt_l2cap_fixed_ch PROGBITS        0003aa28 02e8e8 000024 00   A  0   0  4
  [ 8] bt_conn_cb_area   PROGBITS        0003aa4c 02e90c 000024 00   A  0   0  4
  [ 9] bt_gatt_service_s PROGBITS        0003aa70 02e930 000018 00   A  0   0  4
  [10] settings_handler_ PROGBITS        0003aa88 02e948 000078 00   A  0   0  4
  [11] log_const_section PROGBITS        0003ab00 02e9c0 000130 00   A  0   0  4
  [12] device_handles    PROGBITS        0003ac30 02eaf0 00001e 00   A  0   0  2
  [13] rodata            PROGBITS        0003ac50 02eb10 004e78 00   A  0   0 16
  [14] .ramfunc          PROGBITS        20000000 0347f0 000000 00   W  0   0  1
  [15] datas             PROGBITS        20000000 033988 000b25 00  WA  0   0  8
  [16] device_states     PROGBITS        20000b28 0344b0 000014 00  WA  0   0  4
  [17] k_timer_area      PROGBITS        20000b40 0344c8 000038 00  WA  0   0  8
  [18] k_mem_slab_area   PROGBITS        20000b78 034500 000080 00  WA  0   0  4
  [19] k_mutex_area      PROGBITS        20000bf8 034580 00003c 00  WA  0   0  4
  [20] k_msgq_area       PROGBITS        20000c34 0345bc 000034 00  WA  0   0  4
  [21] k_sem_area        PROGBITS        20000c68 0345f0 000078 00  WA  0   0  4
  [22] k_queue_area      PROGBITS        20000ce0 034668 00001c 00  WA  0   0  4
  [23] _net_buf_pool_are PROGBITS        20000cfc 034684 00016c 00  WA  0   0  4
  [24] bss               NOBITS          20000e68 034808 003534 00  WA  0   0  8
  [25] noinit            NOBITS          200043a0 034808 00b6c0 00  WA  0   0 32
  [26] .comment          PROGBITS        00000000 0347f0 0343f9 00      0   0  1
  [27] .debug_aranges    PROGBITS        00000000 068bf0 0043c8 00      0   0  8
  [28] .debug_info       PROGBITS        00000000 06cfb8 1e6c67 00      0   0  1
  [29] .debug_abbrev     PROGBITS        00000000 253c1f 023641 00      0   0  1
  [30] .debug_line       PROGBITS        00000000 277260 06bbc1 00      0   0  1
  [31] .debug_frame      PROGBITS        00000000 2e2e24 00cba8 00      0   0  4
  [32] .debug_str        PROGBITS        00000000 2ef9cc 020f16 01  MS  0   0  1
  [33] .debug_loc        PROGBITS        00000000 3108e2 07034f 00      0   0  1
  [34] .debug_ranges     PROGBITS        00000000 380c38 014330 00      0   0  8
  [35] .ARM.attributes   ARM_ATTRIBUTES  00000000 394f68 000035 00      0   0  1
  [36] .symtab           SYMTAB          00000000 394fa0 0205a0 10     37 6028  4
  [37] .strtab           STRTAB          00000000 3b5540 013051 00      0   0  1
  [38] .shstrtab         STRTAB          00000000 3c8591 0001e7 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x02e6b0 0x0003a7f0 0x0003a7f0 0x00008 0x00008 R   0x4
  LOAD           0x0000c0 0x0000c200 0x0000c200 0x338c8 0x338c8 RWE 0x10
  LOAD           0x033988 0x20000000 0x0003fac8 0x00e68 0x00e68 RW  0x8
  LOAD           0x034808 0x20000e68 0x20000e68 0x00000 0x0ebf8 RW  0x20

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table bt_l2cap_fixed_chan_area bt_conn_cb_area bt_gatt_service_static_area settings_handler_static_area log_const_sections device_handles rodata 
   02     datas device_states k_timer_area k_mem_slab_area k_mutex_area k_msgq_area k_sem_area k_queue_area _net_buf_pool_area 
   03     bss noinit 
