ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x2305
  Start of program headers:          52 (bytes into file)
  Start of section headers:          921988 (bytes into file)
  Flags:                             0x5000200, Version5 EABI, soft-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         4
  Size of section headers:           40 (bytes)
  Number of section headers:         28
  Section header string table index: 27

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 0000c0 0000dc 00 WAX  0   0  4
  [ 2] text              PROGBITS        000000dc 00019c 006350 00  AX  0   0  4
  [ 3] .ARM.exidx        ARM_EXIDX       0000642c 0064ec 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        00006434 0064f4 000040 00   A  0   0  4
  [ 5] devices           PROGBITS        00006474 006534 000060 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        000064d4 006594 000138 00  WA  0   0  4
  [ 7] log_const_se[...] PROGBITS        0000660c 0066cc 000040 00   A  0   0  4
  [ 8] device_handles    PROGBITS        0000664c 00670c 000018 00   A  0   0  2
  [ 9] rodata            PROGBITS        00006670 006730 000fcc 00   A  0   0 16
  [10] .ramfunc          PROGBITS        20000000 0077a4 000000 00   W  0   0  1
  [11] datas             PROGBITS        20000000 0076fc 000098 00  WA  0   0  4
  [12] device_states     PROGBITS        20000098 007794 000010 00  WA  0   0  4
  [13] bss               NOBITS          200000a8 0077a8 001367 00  WA  0   0  8
  [14] noinit            NOBITS          20001420 0077a8 003040 00  WA  0   0 32
  [15] .comment          PROGBITS        00000000 0077a4 000020 01  MS  0   0  1
  [16] .debug_aranges    PROGBITS        00000000 0077c8 001818 00      0   0  8
  [17] .debug_info       PROGBITS        00000000 008fe0 06d07d 00      0   0  1
  [18] .debug_abbrev     PROGBITS        00000000 07605d 00ccc1 00      0   0  1
  [19] .debug_line       PROGBITS        00000000 082d1e 01cd96 00      0   0  1
  [20] .debug_frame      PROGBITS        00000000 09fab4 003844 00      0   0  4
  [21] .debug_str        PROGBITS        00000000 0a32f8 00c2c5 01  MS  0   0  1
  [22] .debug_loc        PROGBITS        00000000 0af5bd 01f3aa 00      0   0  1
  [23] .debug_ranges     PROGBITS        00000000 0ce968 006218 00      0   0  8
  [24] .ARM.attributes   ARM_ATTRIBUTES  00000000 0d4b80 000033 00      0   0  1
  [25] .symtab           SYMTAB          00000000 0d4bb4 006980 10     26 882  4
  [26] .strtab           STRTAB          00000000 0db534 005b2b 00      0   0  1
  [27] .shstrtab         STRTAB          00000000 0e105f 000124 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x0064ec 0x0000642c 0x0000642c 0x00008 0x00008 R   0x4
  LOAD           0x0000c0 0x00000000 0x00000000 0x0763c 0x0763c RWE 0x10
  LOAD           0x0076fc 0x20000000 0x0000763c 0x000a8 0x000a8 RW  0x4
  LOAD           0x000000 0x200000a8 0x200000a8 0x00000 0x043b8 RW  0x20

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table log_const_sections device_handles rodata 
   02     datas device_states 
   03     bss noinit 
