// This IDL was generated automatically by ZAP.
// It is for view/code review purposes only.

server cluster Descriptor = 29 {
  struct DeviceTypeStruct {
    devtype_id type = 0;
    int16u revision = 1;
  }

  readonly attribute DeviceTypeStruct deviceTypeList[] = 0;
  readonly attribute CLUSTER_ID serverList[] = 1;
  readonly attribute CLUSTER_ID clientList[] = 2;
  readonly attribute ENDPOINT_NO partsList[] = 3;
  readonly attribute command_id generatedCommandList[] = 65528;
  readonly attribute command_id acceptedCommandList[] = 65529;
  readonly attribute attrib_id attributeList[] = 65531;
  readonly attribute bitmap32 featureMap = 65532;
  readonly attribute int16u clusterRevision = 65533;
}

server cluster AccessControl = 31 {
  enum AuthMode : ENUM8 {
    kPase = 1;
    kCase = 2;
    kGroup = 3;
  }

  enum ChangeTypeEnum : ENUM8 {
    kChanged = 0;
    kAdded = 1;
    kRemoved = 2;
  }

  enum Privilege : ENUM8 {
    kView = 1;
    kProxyView = 2;
    kOperate = 3;
    kManage = 4;
    kAdminister = 5;
  }

  fabric_scoped struct AccessControlEntry {
    fabric_sensitive Privilege privilege = 1;
    fabric_sensitive AuthMode authMode = 2;
    nullable fabric_sensitive int64u subjects[] = 3;
    nullable fabric_sensitive Target targets[] = 4;
    fabric_idx fabricIndex = 254;
  }

  struct Target {
    nullable cluster_id cluster = 0;
    nullable endpoint_no endpoint = 1;
    nullable devtype_id deviceType = 2;
  }

  fabric_scoped struct ExtensionEntry {
    fabric_sensitive octet_string<128> data = 1;
    fabric_idx fabricIndex = 254;
  }

  fabric_sensitive info event access(read: administer) AccessControlEntryChanged = 0 {
    nullable node_id adminNodeID = 1;
    nullable INT16U adminPasscodeID = 2;
    ChangeTypeEnum changeType = 3;
    nullable AccessControlEntry latestValue = 4;
    fabric_idx fabricIndex = 254;
  }

  fabric_sensitive info event access(read: administer) AccessControlExtensionChanged = 1 {
    nullable node_id adminNodeID = 1;
    nullable INT16U adminPasscodeID = 2;
    ChangeTypeEnum changeType = 3;
    nullable ExtensionEntry latestValue = 4;
    fabric_idx fabricIndex = 254;
  }

  attribute access(read: administer, write: administer) AccessControlEntry acl[] = 0;
  attribute access(read: administer, write: administer) ExtensionEntry extension[] = 1;
  readonly attribute int16u subjectsPerAccessControlEntry = 2;
  readonly attribute int16u targetsPerAccessControlEntry = 3;
  readonly attribute int16u accessControlEntriesPerFabric = 4;
  readonly attribute command_id generatedCommandList[] = 65528;
  readonly attribute command_id acceptedCommandList[] = 65529;
  readonly attribute attrib_id attributeList[] = 65531;
  readonly attribute bitmap32 featureMap = 65532;
  readonly attribute int16u clusterRevision = 65533;
}

server cluster Basic = 40 {
  struct CapabilityMinimaStruct {
    int16u caseSessionsPerFabric = 0;
    int16u subscriptionsPerFabric = 1;
  }

  critical event StartUp = 0 {
    INT32U softwareVersion = 0;
  }

  critical event ShutDown = 1 {
  }

  info event Leave = 2 {
    fabric_idx fabricIndex = 0;
  }

  info event ReachableChanged = 3 {
    boolean reachableNewValue = 0;
  }

  readonly attribute int16u dataModelRevision = 0;
  readonly attribute char_string<32> vendorName = 1;
  readonly attribute vendor_id vendorID = 2;
  readonly attribute char_string<32> productName = 3;
  readonly attribute int16u productID = 4;
  attribute access(write: manage) char_string<32> nodeLabel = 5;
  attribute access(write: administer) char_string<2> location = 6;
  readonly attribute int16u hardwareVersion = 7;
  readonly attribute char_string<64> hardwareVersionString = 8;
  readonly attribute int32u softwareVersion = 9;
  readonly attribute char_string<64> softwareVersionString = 10;
  readonly attribute char_string<16> manufacturingDate = 11;
  readonly attribute char_string<32> serialNumber = 15;
  readonly attribute char_string<32> uniqueID = 18;
  readonly attribute CapabilityMinimaStruct capabilityMinima = 19;
  readonly attribute command_id generatedCommandList[] = 65528;
  readonly attribute command_id acceptedCommandList[] = 65529;
  readonly attribute attrib_id attributeList[] = 65531;
  readonly attribute bitmap32 featureMap = 65532;
  readonly attribute int16u clusterRevision = 65533;
}

client cluster OtaSoftwareUpdateProvider = 41 {
  enum OTAApplyUpdateAction : ENUM8 {
    kProceed = 0;
    kAwaitNextAction = 1;
    kDiscontinue = 2;
  }

  enum OTADownloadProtocol : ENUM8 {
    kBDXSynchronous = 0;
    kBDXAsynchronous = 1;
    kHttps = 2;
    kVendorSpecific = 3;
  }

  enum OTAQueryStatus : ENUM8 {
    kUpdateAvailable = 0;
    kBusy = 1;
    kNotAvailable = 2;
    kDownloadProtocolNotSupported = 3;
  }


  request struct QueryImageRequest {
    vendor_id vendorId = 0;
    INT16U productId = 1;
    INT32U softwareVersion = 2;
    OTADownloadProtocol protocolsSupported[] = 3;
    optional INT16U hardwareVersion = 4;
    optional CHAR_STRING<2> location = 5;
    optional BOOLEAN requestorCanConsent = 6;
    optional OCTET_STRING<512> metadataForProvider = 7;
  }

  request struct ApplyUpdateRequestRequest {
    OCTET_STRING<32> updateToken = 0;
    INT32U newVersion = 1;
  }

  request struct NotifyUpdateAppliedRequest {
    OCTET_STRING<32> updateToken = 0;
    INT32U softwareVersion = 1;
  }

  response struct QueryImageResponse = 1 {
    OTAQueryStatus status = 0;
    optional INT32U delayedActionTime = 1;
    optional CHAR_STRING<256> imageURI = 2;
    optional INT32U softwareVersion = 3;
    optional CHAR_STRING<64> softwareVersionString = 4;
    optional OCTET_STRING<32> updateToken = 5;
    optional BOOLEAN userConsentNeeded = 6;
    optional OCTET_STRING<512> metadataForRequestor = 7;
  }

  response struct ApplyUpdateResponse = 3 {
    OTAApplyUpdateAction action = 0;
    INT32U delayedActionTime = 1;
  }

  command QueryImage(QueryImageRequest): QueryImageResponse = 0;
  command ApplyUpdateRequest(ApplyUpdateRequestRequest): ApplyUpdateResponse = 2;
  command NotifyUpdateApplied(NotifyUpdateAppliedRequest): DefaultSuccess = 4;
}

server cluster OtaSoftwareUpdateRequestor = 42 {
  enum OTAAnnouncementReason : ENUM8 {
    kSimpleAnnouncement = 0;
    kUpdateAvailable = 1;
    kUrgentUpdateAvailable = 2;
  }

  enum OTAChangeReasonEnum : ENUM8 {
    kUnknown = 0;
    kSuccess = 1;
    kFailure = 2;
    kTimeOut = 3;
    kDelayByProvider = 4;
  }

  enum OTAUpdateStateEnum : ENUM8 {
    kUnknown = 0;
    kIdle = 1;
    kQuerying = 2;
    kDelayedOnQuery = 3;
    kDownloading = 4;
    kApplying = 5;
    kDelayedOnApply = 6;
    kRollingBack = 7;
    kDelayedOnUserConsent = 8;
  }

  fabric_scoped struct ProviderLocation {
    node_id providerNodeID = 1;
    endpoint_no endpoint = 2;
    fabric_idx fabricIndex = 254;
  }

  info event StateTransition = 0 {
    OTAUpdateStateEnum previousState = 0;
    OTAUpdateStateEnum newState = 1;
    OTAChangeReasonEnum reason = 2;
    nullable INT32U targetSoftwareVersion = 3;
  }

  critical event VersionApplied = 1 {
    INT32U softwareVersion = 0;
    INT16U productID = 1;
  }

  info event DownloadError = 2 {
    INT32U softwareVersion = 0;
    INT64U bytesDownloaded = 1;
    nullable INT8U progressPercent = 2;
    nullable INT64S platformCode = 3;
  }

  attribute ProviderLocation defaultOtaProviders[] = 0;
  readonly attribute boolean updatePossible = 1;
  readonly attribute OTAUpdateStateEnum updateState = 2;
  readonly attribute nullable int8u updateStateProgress = 3;
  readonly attribute command_id generatedCommandList[] = 65528;
  readonly attribute command_id acceptedCommandList[] = 65529;
  readonly attribute attrib_id attributeList[] = 65531;
  readonly attribute bitmap32 featureMap = 65532;
  readonly attribute int16u clusterRevision = 65533;

  request struct AnnounceOtaProviderRequest {
    node_id providerNodeId = 0;
    vendor_id vendorId = 1;
    OTAAnnouncementReason announcementReason = 2;
    optional OCTET_STRING<512> metadataForNode = 3;
    endpoint_no endpoint = 4;
  }

  command AnnounceOtaProvider(AnnounceOtaProviderRequest): DefaultSuccess = 0;
}

server cluster GeneralCommissioning = 48 {
  enum CommissioningError : ENUM8 {
    kOk = 0;
    kValueOutsideRange = 1;
    kInvalidAuthentication = 2;
    kNoFailSafe = 3;
    kBusyWithOtherAdmin = 4;
  }

  enum RegulatoryLocationType : ENUM8 {
    kIndoor = 0;
    kOutdoor = 1;
    kIndoorOutdoor = 2;
  }

  struct BasicCommissioningInfo {
    int16u failSafeExpiryLengthSeconds = 0;
    int16u maxCumulativeFailsafeSeconds = 1;
  }

  attribute access(write: administer) int64u breadcrumb = 0;
  readonly attribute BasicCommissioningInfo basicCommissioningInfo = 1;
  readonly attribute RegulatoryLocationType regulatoryConfig = 2;
  readonly attribute RegulatoryLocationType locationCapability = 3;
  readonly attribute boolean supportsConcurrentConnection = 4;
  readonly attribute command_id generatedCommandList[] = 65528;
  readonly attribute command_id acceptedCommandList[] = 65529;
  readonly attribute attrib_id attributeList[] = 65531;
  readonly attribute bitmap32 featureMap = 65532;
  readonly attribute int16u clusterRevision = 65533;

  request struct ArmFailSafeRequest {
    INT16U expiryLengthSeconds = 0;
    INT64U breadcrumb = 1;
  }

  request struct SetRegulatoryConfigRequest {
    RegulatoryLocationType newRegulatoryConfig = 0;
    CHAR_STRING countryCode = 1;
    INT64U breadcrumb = 2;
  }

  response struct ArmFailSafeResponse = 1 {
    CommissioningError errorCode = 0;
    CHAR_STRING debugText = 1;
  }

  response struct SetRegulatoryConfigResponse = 3 {
    CommissioningError errorCode = 0;
    CHAR_STRING debugText = 1;
  }

  response struct CommissioningCompleteResponse = 5 {
    CommissioningError errorCode = 0;
    CHAR_STRING debugText = 1;
  }

  command access(invoke: administer) ArmFailSafe(ArmFailSafeRequest): ArmFailSafeResponse = 0;
  command access(invoke: administer) SetRegulatoryConfig(SetRegulatoryConfigRequest): SetRegulatoryConfigResponse = 2;
  fabric command access(invoke: administer) CommissioningComplete(): CommissioningCompleteResponse = 4;
}

server cluster NetworkCommissioning = 49 {
  enum NetworkCommissioningStatus : ENUM8 {
    kSuccess = 0;
    kOutOfRange = 1;
    kBoundsExceeded = 2;
    kNetworkIDNotFound = 3;
    kDuplicateNetworkID = 4;
    kNetworkNotFound = 5;
    kRegulatoryError = 6;
    kAuthFailure = 7;
    kUnsupportedSecurity = 8;
    kOtherConnectionFailure = 9;
    kIPV6Failed = 10;
    kIPBindFailed = 11;
    kUnknownError = 12;
  }

  enum WiFiBand : ENUM8 {
    k2g4 = 0;
    k3g65 = 1;
    k5g = 2;
    k6g = 3;
    k60g = 4;
  }

  bitmap NetworkCommissioningFeature : BITMAP32 {
    kWiFiNetworkInterface = 0x1;
    kThreadNetworkInterface = 0x2;
    kEthernetNetworkInterface = 0x4;
  }

  bitmap WiFiSecurity : BITMAP8 {
    kUnencrypted = 0x1;
    kWepPersonal = 0x2;
    kWpaPersonal = 0x4;
    kWpa2Personal = 0x8;
    kWpa3Personal = 0x10;
  }

  struct NetworkInfo {
    octet_string<32> networkID = 0;
    boolean connected = 1;
  }

  struct WiFiInterfaceScanResult {
    WiFiSecurity security = 0;
    octet_string<32> ssid = 1;
    octet_string<6> bssid = 2;
    int16u channel = 3;
    WiFiBand wiFiBand = 4;
    int8s rssi = 5;
  }

  struct ThreadInterfaceScanResult {
    int16u panId = 0;
    int64u extendedPanId = 1;
    char_string<16> networkName = 2;
    int16u channel = 3;
    int8u version = 4;
    octet_string<8> extendedAddress = 5;
    int8s rssi = 6;
    int8u lqi = 7;
  }

  readonly attribute access(read: administer) int8u maxNetworks = 0;
  readonly attribute access(read: administer) NetworkInfo networks[] = 1;
  readonly attribute int8u scanMaxTimeSeconds = 2;
  readonly attribute int8u connectMaxTimeSeconds = 3;
  attribute access(write: administer) boolean interfaceEnabled = 4;
  readonly attribute access(read: administer) nullable NetworkCommissioningStatus lastNetworkingStatus = 5;
  readonly attribute access(read: administer) nullable octet_string<32> lastNetworkID = 6;
  readonly attribute access(read: administer) nullable int32s lastConnectErrorValue = 7;
  readonly attribute command_id generatedCommandList[] = 65528;
  readonly attribute command_id acceptedCommandList[] = 65529;
  readonly attribute attrib_id attributeList[] = 65531;
  readonly attribute bitmap32 featureMap = 65532;
  readonly attribute int16u clusterRevision = 65533;

  request struct ScanNetworksRequest {
    optional nullable OCTET_STRING<32> ssid = 0;
    optional INT64U breadcrumb = 1;
  }

  request struct AddOrUpdateWiFiNetworkRequest {
    OCTET_STRING<32> ssid = 0;
    OCTET_STRING<64> credentials = 1;
    optional INT64U breadcrumb = 2;
  }

  request struct AddOrUpdateThreadNetworkRequest {
    OCTET_STRING<254> operationalDataset = 0;
    optional INT64U breadcrumb = 1;
  }

  request struct RemoveNetworkRequest {
    OCTET_STRING<32> networkID = 0;
    optional INT64U breadcrumb = 1;
  }

  request struct ConnectNetworkRequest {
    OCTET_STRING<32> networkID = 0;
    optional INT64U breadcrumb = 1;
  }

  request struct ReorderNetworkRequest {
    OCTET_STRING<32> networkID = 0;
    INT8U networkIndex = 1;
    optional INT64U breadcrumb = 2;
  }

  response struct ScanNetworksResponse = 1 {
    NetworkCommissioningStatus networkingStatus = 0;
    optional CHAR_STRING debugText = 1;
    optional WiFiInterfaceScanResult wiFiScanResults[] = 2;
    optional ThreadInterfaceScanResult threadScanResults[] = 3;
  }

  response struct NetworkConfigResponse = 5 {
    NetworkCommissioningStatus networkingStatus = 0;
    optional CHAR_STRING<512> debugText = 1;
    optional INT8U networkIndex = 2;
  }

  response struct ConnectNetworkResponse = 7 {
    NetworkCommissioningStatus networkingStatus = 0;
    optional CHAR_STRING debugText = 1;
    nullable INT32S errorValue = 2;
  }

  command access(invoke: administer) ScanNetworks(ScanNetworksRequest): ScanNetworksResponse = 0;
  command access(invoke: administer) AddOrUpdateWiFiNetwork(AddOrUpdateWiFiNetworkRequest): NetworkConfigResponse = 2;
  command access(invoke: administer) AddOrUpdateThreadNetwork(AddOrUpdateThreadNetworkRequest): NetworkConfigResponse = 3;
  command access(invoke: administer) RemoveNetwork(RemoveNetworkRequest): NetworkConfigResponse = 4;
  command access(invoke: administer) ConnectNetwork(ConnectNetworkRequest): ConnectNetworkResponse = 6;
  command access(invoke: administer) ReorderNetwork(ReorderNetworkRequest): NetworkConfigResponse = 8;
}

server cluster GeneralDiagnostics = 51 {
  enum BootReasonType : ENUM8 {
    kUnspecified = 0;
    kPowerOnReboot = 1;
    kBrownOutReset = 2;
    kSoftwareWatchdogReset = 3;
    kHardwareWatchdogReset = 4;
    kSoftwareUpdateCompleted = 5;
    kSoftwareReset = 6;
  }

  enum HardwareFaultType : ENUM8 {
    kUnspecified = 0;
    kRadio = 1;
    kSensor = 2;
    kResettableOverTemp = 3;
    kNonResettableOverTemp = 4;
    kPowerSource = 5;
    kVisualDisplayFault = 6;
    kAudioOutputFault = 7;
    kUserInterfaceFault = 8;
    kNonVolatileMemoryError = 9;
    kTamperDetected = 10;
  }

  enum InterfaceType : ENUM8 {
    kUnspecified = 0;
    kWiFi = 1;
    kEthernet = 2;
    kCellular = 3;
    kThread = 4;
  }

  enum NetworkFaultType : ENUM8 {
    kUnspecified = 0;
    kHardwareFailure = 1;
    kNetworkJammed = 2;
    kConnectionFailed = 3;
  }

  enum RadioFaultType : ENUM8 {
    kUnspecified = 0;
    kWiFiFault = 1;
    kCellularFault = 2;
    kThreadFault = 3;
    kNFCFault = 4;
    kBLEFault = 5;
    kEthernetFault = 6;
  }

  struct NetworkInterfaceType {
    char_string<32> name = 0;
    boolean isOperational = 1;
    nullable boolean offPremiseServicesReachableIPv4 = 2;
    nullable boolean offPremiseServicesReachableIPv6 = 3;
    octet_string<8> hardwareAddress = 4;
    octet_string IPv4Addresses[] = 5;
    octet_string IPv6Addresses[] = 6;
    InterfaceType type = 7;
  }

  critical event HardwareFaultChange = 0 {
    HardwareFaultType current[] = 0;
    HardwareFaultType previous[] = 1;
  }

  critical event RadioFaultChange = 1 {
    RadioFaultType current[] = 0;
    RadioFaultType previous[] = 1;
  }

  critical event NetworkFaultChange = 2 {
    NetworkFaultType current[] = 0;
    NetworkFaultType previous[] = 1;
  }

  critical event BootReason = 3 {
    BootReasonType bootReason = 0;
  }

  readonly attribute NetworkInterfaceType networkInterfaces[] = 0;
  readonly attribute int16u rebootCount = 1;
  readonly attribute int64u upTime = 2;
  readonly attribute int32u totalOperationalHours = 3;
  readonly attribute enum8 bootReasons = 4;
  readonly attribute boolean testEventTriggersEnabled = 8;
  readonly attribute command_id generatedCommandList[] = 65528;
  readonly attribute command_id acceptedCommandList[] = 65529;
  readonly attribute attrib_id attributeList[] = 65531;
  readonly attribute bitmap32 featureMap = 65532;
  readonly attribute int16u clusterRevision = 65533;

  request struct TestEventTriggerRequest {
    OCTET_STRING<16> enableKey = 0;
    INT64U eventTrigger = 1;
  }

  command access(invoke: manage) TestEventTrigger(TestEventTriggerRequest): DefaultSuccess = 0;
}

server cluster SoftwareDiagnostics = 52 {
  bitmap SoftwareDiagnosticsFeature : BITMAP32 {
    kWaterMarks = 0x1;
  }

  info event SoftwareFault = 0 {
    INT64U id = 0;
    optional CHAR_STRING name = 1;
    optional OCTET_STRING faultRecording = 2;
  }

  readonly attribute int64u currentHeapFree = 1;
  readonly attribute int64u currentHeapUsed = 2;
  readonly attribute command_id generatedCommandList[] = 65528;
  readonly attribute command_id acceptedCommandList[] = 65529;
  readonly attribute attrib_id attributeList[] = 65531;
  readonly attribute bitmap32 featureMap = 65532;
  readonly attribute int16u clusterRevision = 65533;
}

server cluster ThreadNetworkDiagnostics = 53 {
  enum NetworkFault : ENUM8 {
    kUnspecified = 0;
    kLinkDown = 1;
    kHardwareFailure = 2;
    kNetworkJammed = 3;
  }

  enum RoutingRole : ENUM8 {
    kUnspecified = 0;
    kUnassigned = 1;
    kSleepyEndDevice = 2;
    kEndDevice = 3;
    kReed = 4;
    kRouter = 5;
    kLeader = 6;
  }

  enum ThreadConnectionStatus : ENUM8 {
    kConnected = 0;
    kNotConnected = 1;
  }

  bitmap ThreadNetworkDiagnosticsFeature : BITMAP32 {
    kPacketCounts = 0x1;
    kErrorCounts = 0x2;
    kMLECounts = 0x4;
    kMACCounts = 0x8;
  }

  struct NeighborTable {
    int64u extAddress = 0;
    int32u age = 1;
    int16u rloc16 = 2;
    int32u linkFrameCounter = 3;
    int32u mleFrameCounter = 4;
    int8u lqi = 5;
    nullable int8s averageRssi = 6;
    nullable int8s lastRssi = 7;
    int8u frameErrorRate = 8;
    int8u messageErrorRate = 9;
    boolean rxOnWhenIdle = 10;
    boolean fullThreadDevice = 11;
    boolean fullNetworkData = 12;
    boolean isChild = 13;
  }

  struct RouteTable {
    int64u extAddress = 0;
    int16u rloc16 = 1;
    int8u routerId = 2;
    int8u nextHop = 3;
    int8u pathCost = 4;
    int8u LQIIn = 5;
    int8u LQIOut = 6;
    int8u age = 7;
    boolean allocated = 8;
    boolean linkEstablished = 9;
  }

  struct SecurityPolicy {
    int16u rotationTime = 0;
    bitmap16 flags = 1;
  }

  struct OperationalDatasetComponents {
    boolean activeTimestampPresent = 0;
    boolean pendingTimestampPresent = 1;
    boolean masterKeyPresent = 2;
    boolean networkNamePresent = 3;
    boolean extendedPanIdPresent = 4;
    boolean meshLocalPrefixPresent = 5;
    boolean delayPresent = 6;
    boolean panIdPresent = 7;
    boolean channelPresent = 8;
    boolean pskcPresent = 9;
    boolean securityPolicyPresent = 10;
    boolean channelMaskPresent = 11;
  }

  info event ConnectionStatus = 0 {
    ThreadConnectionStatus connectionStatus = 0;
  }

  info event NetworkFaultChange = 1 {
    NetworkFault current[] = 0;
    NetworkFault previous[] = 1;
  }

  readonly attribute nullable int16u channel = 0;
  readonly attribute nullable RoutingRole routingRole = 1;
  readonly attribute nullable char_string<16> networkName = 2;
  readonly attribute nullable int16u panId = 3;
  readonly attribute nullable int64u extendedPanId = 4;
  readonly attribute nullable octet_string<17> meshLocalPrefix = 5;
  readonly attribute int64u overrunCount = 6;
  readonly attribute NeighborTable neighborTableList[] = 7;
  readonly attribute RouteTable routeTableList[] = 8;
  readonly attribute nullable int32u partitionId = 9;
  readonly attribute nullable int8u weighting = 10;
  readonly attribute nullable int8u dataVersion = 11;
  readonly attribute nullable int8u stableDataVersion = 12;
  readonly attribute nullable int8u leaderRouterId = 13;
  readonly attribute int16u detachedRoleCount = 14;
  readonly attribute int16u childRoleCount = 15;
  readonly attribute int16u routerRoleCount = 16;
  readonly attribute int16u leaderRoleCount = 17;
  readonly attribute int16u attachAttemptCount = 18;
  readonly attribute int16u partitionIdChangeCount = 19;
  readonly attribute int16u betterPartitionAttachAttemptCount = 20;
  readonly attribute int16u parentChangeCount = 21;
  readonly attribute int32u txTotalCount = 22;
  readonly attribute int32u txUnicastCount = 23;
  readonly attribute int32u txBroadcastCount = 24;
  readonly attribute int32u txAckRequestedCount = 25;
  readonly attribute int32u txAckedCount = 26;
  readonly attribute int32u txNoAckRequestedCount = 27;
  readonly attribute int32u txDataCount = 28;
  readonly attribute int32u txDataPollCount = 29;
  readonly attribute int32u txBeaconCount = 30;
  readonly attribute int32u txBeaconRequestCount = 31;
  readonly attribute int32u txOtherCount = 32;
  readonly attribute int32u txRetryCount = 33;
  readonly attribute int32u txDirectMaxRetryExpiryCount = 34;
  readonly attribute int32u txIndirectMaxRetryExpiryCount = 35;
  readonly attribute int32u txErrCcaCount = 36;
  readonly attribute int32u txErrAbortCount = 37;
  readonly attribute int32u txErrBusyChannelCount = 38;
  readonly attribute int32u rxTotalCount = 39;
  readonly attribute int32u rxUnicastCount = 40;
  readonly attribute int32u rxBroadcastCount = 41;
  readonly attribute int32u rxDataCount = 42;
  readonly attribute int32u rxDataPollCount = 43;
  readonly attribute int32u rxBeaconCount = 44;
  readonly attribute int32u rxBeaconRequestCount = 45;
  readonly attribute int32u rxOtherCount = 46;
  readonly attribute int32u rxAddressFilteredCount = 47;
  readonly attribute int32u rxDestAddrFilteredCount = 48;
  readonly attribute int32u rxDuplicatedCount = 49;
  readonly attribute int32u rxErrNoFrameCount = 50;
  readonly attribute int32u rxErrUnknownNeighborCount = 51;
  readonly attribute int32u rxErrInvalidSrcAddrCount = 52;
  readonly attribute int32u rxErrSecCount = 53;
  readonly attribute int32u rxErrFcsCount = 54;
  readonly attribute int32u rxErrOtherCount = 55;
  readonly attribute nullable int64u activeTimestamp = 56;
  readonly attribute nullable int64u pendingTimestamp = 57;
  readonly attribute nullable int32u delay = 58;
  readonly attribute nullable SecurityPolicy securityPolicy = 59;
  readonly attribute nullable octet_string<4> channelPage0Mask = 60;
  readonly attribute nullable OperationalDatasetComponents operationalDatasetComponents = 61;
  readonly attribute NetworkFault activeNetworkFaultsList[] = 62;
  readonly attribute command_id generatedCommandList[] = 65528;
  readonly attribute command_id acceptedCommandList[] = 65529;
  readonly attribute attrib_id attributeList[] = 65531;
  readonly attribute bitmap32 featureMap = 65532;
  readonly attribute int16u clusterRevision = 65533;

  command ResetCounts(): DefaultSuccess = 0;
}

server cluster WiFiNetworkDiagnostics = 54 {
  enum AssociationFailureCause : ENUM8 {
    kUnknown = 0;
    kAssociationFailed = 1;
    kAuthenticationFailed = 2;
    kSsidNotFound = 3;
  }

  enum SecurityType : ENUM8 {
    kUnspecified = 0;
    kNone = 1;
    kWep = 2;
    kWpa = 3;
    kWpa2 = 4;
    kWpa3 = 5;
  }

  enum WiFiConnectionStatus : ENUM8 {
    kConnected = 0;
    kNotConnected = 1;
  }

  enum WiFiVersionType : ENUM8 {
    k80211a = 0;
    k80211b = 1;
    k80211g = 2;
    k80211n = 3;
    k80211ac = 4;
    k80211ax = 5;
  }

  info event Disconnection = 0 {
    INT16U reasonCode = 0;
  }

  info event AssociationFailure = 1 {
    AssociationFailureCause associationFailure = 0;
    INT16U status = 1;
  }

  info event ConnectionStatus = 2 {
    WiFiConnectionStatus connectionStatus = 0;
  }

  readonly attribute nullable octet_string<6> bssid = 0;
  readonly attribute nullable SecurityType securityType = 1;
  readonly attribute nullable WiFiVersionType wiFiVersion = 2;
  readonly attribute nullable int16u channelNumber = 3;
  readonly attribute nullable int8s rssi = 4;
  readonly attribute nullable int32u beaconLostCount = 5;
  readonly attribute nullable int32u beaconRxCount = 6;
  readonly attribute nullable int32u packetMulticastRxCount = 7;
  readonly attribute nullable int32u packetMulticastTxCount = 8;
  readonly attribute nullable int32u packetUnicastRxCount = 9;
  readonly attribute nullable int32u packetUnicastTxCount = 10;
  readonly attribute nullable int64u currentMaxRate = 11;
  readonly attribute nullable int64u overrunCount = 12;
  readonly attribute command_id generatedCommandList[] = 65528;
  readonly attribute command_id acceptedCommandList[] = 65529;
  readonly attribute attrib_id attributeList[] = 65531;
  readonly attribute bitmap32 featureMap = 65532;
  readonly attribute int16u clusterRevision = 65533;

  command ResetCounts(): DefaultSuccess = 0;
}

server cluster AdministratorCommissioning = 60 {
  enum CommissioningWindowStatus : ENUM8 {
    kWindowNotOpen = 0;
    kEnhancedWindowOpen = 1;
    kBasicWindowOpen = 2;
  }

  enum StatusCode : ENUM8 {
    kBusy = 2;
    kPAKEParameterError = 3;
    kWindowNotOpen = 4;
  }

  readonly attribute CommissioningWindowStatus windowStatus = 0;
  readonly attribute nullable fabric_idx adminFabricIndex = 1;
  readonly attribute nullable int16u adminVendorId = 2;
  readonly attribute command_id generatedCommandList[] = 65528;
  readonly attribute command_id acceptedCommandList[] = 65529;
  readonly attribute attrib_id attributeList[] = 65531;
  readonly attribute bitmap32 featureMap = 65532;
  readonly attribute int16u clusterRevision = 65533;

  request struct OpenCommissioningWindowRequest {
    INT16U commissioningTimeout = 0;
    OCTET_STRING PAKEVerifier = 1;
    INT16U discriminator = 2;
    INT32U iterations = 3;
    OCTET_STRING salt = 4;
  }

  request struct OpenBasicCommissioningWindowRequest {
    INT16U commissioningTimeout = 0;
  }

  timed command access(invoke: administer) OpenCommissioningWindow(OpenCommissioningWindowRequest): DefaultSuccess = 0;
  timed command access(invoke: administer) OpenBasicCommissioningWindow(OpenBasicCommissioningWindowRequest): DefaultSuccess = 1;
  timed command access(invoke: administer) RevokeCommissioning(): DefaultSuccess = 2;
}

server cluster OperationalCredentials = 62 {
  enum OperationalCertStatus : ENUM8 {
    kSuccess = 0;
    kInvalidPublicKey = 1;
    kInvalidNodeOpId = 2;
    kInvalidNOC = 3;
    kMissingCsr = 4;
    kTableFull = 5;
    kInvalidAdminSubject = 6;
    kFabricConflict = 9;
    kLabelConflict = 10;
    kInvalidFabricIndex = 11;
  }

  fabric_scoped struct NOCStruct {
    fabric_sensitive octet_string noc = 1;
    nullable fabric_sensitive octet_string icac = 2;
    fabric_idx fabricIndex = 254;
  }

  fabric_scoped struct FabricDescriptor {
    octet_string<65> rootPublicKey = 1;
    vendor_id vendorId = 2;
    fabric_id fabricId = 3;
    node_id nodeId = 4;
    char_string<32> label = 5;
    fabric_idx fabricIndex = 254;
  }

  readonly attribute access(read: administer) NOCStruct NOCs[] = 0;
  readonly attribute FabricDescriptor fabrics[] = 1;
  readonly attribute int8u supportedFabrics = 2;
  readonly attribute int8u commissionedFabrics = 3;
  readonly attribute OCTET_STRING trustedRootCertificates[] = 4;
  readonly attribute int8u currentFabricIndex = 5;
  readonly attribute command_id generatedCommandList[] = 65528;
  readonly attribute command_id acceptedCommandList[] = 65529;
  readonly attribute attrib_id attributeList[] = 65531;
  readonly attribute bitmap32 featureMap = 65532;
  readonly attribute int16u clusterRevision = 65533;

  request struct AttestationRequestRequest {
    OCTET_STRING attestationNonce = 0;
  }

  request struct CertificateChainRequestRequest {
    INT8U certificateType = 0;
  }

  request struct CSRRequestRequest {
    OCTET_STRING CSRNonce = 0;
    optional boolean isForUpdateNOC = 1;
  }

  request struct AddNOCRequest {
    OCTET_STRING NOCValue = 0;
    optional OCTET_STRING ICACValue = 1;
    OCTET_STRING IPKValue = 2;
    Int64u caseAdminSubject = 3;
    VENDOR_ID adminVendorId = 4;
  }

  request struct UpdateNOCRequest {
    OCTET_STRING NOCValue = 0;
    optional OCTET_STRING ICACValue = 1;
  }

  request struct UpdateFabricLabelRequest {
    CHAR_STRING<32> label = 0;
  }

  request struct RemoveFabricRequest {
    fabric_idx fabricIndex = 0;
  }

  request struct AddTrustedRootCertificateRequest {
    OCTET_STRING rootCertificate = 0;
  }

  response struct AttestationResponse = 1 {
    OCTET_STRING attestationElements = 0;
    OCTET_STRING signature = 1;
  }

  response struct CertificateChainResponse = 3 {
    OCTET_STRING certificate = 0;
  }

  response struct CSRResponse = 5 {
    OCTET_STRING NOCSRElements = 0;
    OCTET_STRING attestationSignature = 1;
  }

  response struct NOCResponse = 8 {
    OperationalCertStatus statusCode = 0;
    optional fabric_idx fabricIndex = 1;
    optional CHAR_STRING debugText = 2;
  }

  command access(invoke: administer) AttestationRequest(AttestationRequestRequest): AttestationResponse = 0;
  command access(invoke: administer) CertificateChainRequest(CertificateChainRequestRequest): CertificateChainResponse = 2;
  command access(invoke: administer) CSRRequest(CSRRequestRequest): CSRResponse = 4;
  command access(invoke: administer) AddNOC(AddNOCRequest): NOCResponse = 6;
  fabric command access(invoke: administer) UpdateNOC(UpdateNOCRequest): NOCResponse = 7;
  fabric command access(invoke: administer) UpdateFabricLabel(UpdateFabricLabelRequest): NOCResponse = 9;
  command access(invoke: administer) RemoveFabric(RemoveFabricRequest): NOCResponse = 10;
  command access(invoke: administer) AddTrustedRootCertificate(AddTrustedRootCertificateRequest): DefaultSuccess = 11;
}

server cluster GroupKeyManagement = 63 {
  enum GroupKeySecurityPolicy : ENUM8 {
    kTrustFirst = 0;
    kCacheAndSync = 1;
  }

  fabric_scoped struct GroupKeyMapStruct {
    group_id groupId = 1;
    int16u groupKeySetID = 2;
    fabric_idx fabricIndex = 254;
  }

  fabric_scoped struct GroupInfoMapStruct {
    group_id groupId = 1;
    endpoint_no endpoints[] = 2;
    optional char_string<16> groupName = 3;
    fabric_idx fabricIndex = 254;
  }

  struct GroupKeySetStruct {
    int16u groupKeySetID = 0;
    GroupKeySecurityPolicy groupKeySecurityPolicy = 1;
    nullable octet_string<16> epochKey0 = 2;
    nullable epoch_us epochStartTime0 = 3;
    nullable octet_string<16> epochKey1 = 4;
    nullable epoch_us epochStartTime1 = 5;
    nullable octet_string<16> epochKey2 = 6;
    nullable epoch_us epochStartTime2 = 7;
  }

  attribute access(write: manage) GroupKeyMapStruct groupKeyMap[] = 0;
  readonly attribute GroupInfoMapStruct groupTable[] = 1;
  readonly attribute int16u maxGroupsPerFabric = 2;
  readonly attribute int16u maxGroupKeysPerFabric = 3;
  readonly attribute command_id generatedCommandList[] = 65528;
  readonly attribute command_id acceptedCommandList[] = 65529;
  readonly attribute attrib_id attributeList[] = 65531;
  readonly attribute bitmap32 featureMap = 65532;
  readonly attribute int16u clusterRevision = 65533;

  request struct KeySetWriteRequest {
    GroupKeySetStruct groupKeySet = 0;
  }

  request struct KeySetReadRequest {
    INT16U groupKeySetID = 0;
  }

  request struct KeySetRemoveRequest {
    INT16U groupKeySetID = 0;
  }

  request struct KeySetReadAllIndicesRequest {
    INT16U groupKeySetIDs[] = 0;
  }

  response struct KeySetReadResponse = 2 {
    GroupKeySetStruct groupKeySet = 0;
  }

  response struct KeySetReadAllIndicesResponse = 5 {
    INT16U groupKeySetIDs[] = 0;
  }

  fabric command access(invoke: administer) KeySetWrite(KeySetWriteRequest): DefaultSuccess = 0;
  fabric command access(invoke: administer) KeySetRead(KeySetReadRequest): KeySetReadResponse = 1;
  fabric command access(invoke: administer) KeySetRemove(KeySetRemoveRequest): DefaultSuccess = 3;
  fabric command access(invoke: administer) KeySetReadAllIndices(KeySetReadAllIndicesRequest): KeySetReadAllIndicesResponse = 4;
}

endpoint 0 {
  device type rootdevice = 22;
  binding cluster OtaSoftwareUpdateProvider;

  server cluster Descriptor {
    callback attribute deviceTypeList;
    callback attribute serverList;
    callback attribute clientList;
    callback attribute partsList;
    callback attribute generatedCommandList;
    callback attribute acceptedCommandList;
    callback attribute attributeList;
    ram      attribute featureMap;
    callback attribute clusterRevision default = 1;
  }

  server cluster AccessControl {
    callback attribute acl;
    callback attribute extension;
    callback attribute subjectsPerAccessControlEntry default = 4;
    callback attribute targetsPerAccessControlEntry default = 3;
    callback attribute accessControlEntriesPerFabric default = 3;
    callback attribute generatedCommandList;
    callback attribute acceptedCommandList;
    callback attribute attributeList;
    ram      attribute featureMap;
    ram      attribute clusterRevision default = 1;
  }

  server cluster Basic {
    callback attribute dataModelRevision default = 10;
    callback attribute vendorName;
    callback attribute vendorID;
    callback attribute productName;
    callback attribute productID;
    persist  attribute nodeLabel;
    callback attribute location default = "XX";
    callback attribute hardwareVersion;
    callback attribute hardwareVersionString;
    callback attribute softwareVersion;
    callback attribute softwareVersionString;
    callback attribute manufacturingDate default = "20210614123456ZZ";
    callback attribute serialNumber;
    callback attribute uniqueID;
    callback attribute capabilityMinima;
    callback attribute generatedCommandList;
    callback attribute acceptedCommandList;
    callback attribute attributeList;
    ram      attribute featureMap;
    ram      attribute clusterRevision default = 1;
  }

  server cluster OtaSoftwareUpdateRequestor {
    callback attribute defaultOtaProviders;
    ram      attribute updatePossible default = 1;
    ram      attribute updateState;
    ram      attribute updateStateProgress;
    callback attribute generatedCommandList;
    callback attribute acceptedCommandList;
    callback attribute attributeList;
    ram      attribute featureMap;
    ram      attribute clusterRevision default = 1;
  }

  server cluster GeneralCommissioning {
    ram      attribute breadcrumb;
    callback attribute basicCommissioningInfo;
    callback attribute regulatoryConfig;
    callback attribute locationCapability;
    callback attribute supportsConcurrentConnection default = 1;
    callback attribute generatedCommandList;
    callback attribute acceptedCommandList;
    callback attribute attributeList;
    ram      attribute featureMap;
    ram      attribute clusterRevision default = 1;
  }

  server cluster NetworkCommissioning {
    callback attribute maxNetworks;
    callback attribute networks;
    callback attribute scanMaxTimeSeconds;
    callback attribute connectMaxTimeSeconds;
    callback attribute interfaceEnabled;
    callback attribute lastNetworkingStatus;
    callback attribute lastNetworkID;
    callback attribute lastConnectErrorValue;
    callback attribute generatedCommandList;
    callback attribute acceptedCommandList;
    callback attribute attributeList;
    callback attribute featureMap default = 2;
    ram      attribute clusterRevision default = 1;
  }

  server cluster GeneralDiagnostics {
    callback attribute networkInterfaces;
    callback attribute rebootCount;
    callback attribute upTime;
    callback attribute totalOperationalHours;
    callback attribute bootReasons;
    callback attribute testEventTriggersEnabled;
    callback attribute generatedCommandList;
    callback attribute acceptedCommandList;
    callback attribute attributeList;
    ram      attribute featureMap;
    ram      attribute clusterRevision default = 1;
  }

  server cluster SoftwareDiagnostics {
    callback attribute currentHeapFree;
    callback attribute currentHeapUsed;
    callback attribute generatedCommandList;
    callback attribute acceptedCommandList;
    callback attribute attributeList;
    ram      attribute featureMap default = 1;
    ram      attribute clusterRevision default = 1;
  }

  server cluster ThreadNetworkDiagnostics {
    callback attribute channel;
    callback attribute routingRole;
    callback attribute networkName;
    callback attribute panId;
    callback attribute extendedPanId;
    callback attribute meshLocalPrefix;
    callback attribute overrunCount;
    callback attribute neighborTableList;
    callback attribute routeTableList;
    callback attribute partitionId;
    callback attribute weighting;
    callback attribute dataVersion;
    callback attribute stableDataVersion;
    callback attribute leaderRouterId;
    callback attribute detachedRoleCount;
    callback attribute childRoleCount;
    callback attribute routerRoleCount;
    callback attribute leaderRoleCount;
    callback attribute attachAttemptCount;
    callback attribute partitionIdChangeCount;
    callback attribute betterPartitionAttachAttemptCount;
    callback attribute parentChangeCount;
    callback attribute txTotalCount;
    callback attribute txUnicastCount;
    callback attribute txBroadcastCount;
    callback attribute txAckRequestedCount;
    callback attribute txAckedCount;
    callback attribute txNoAckRequestedCount;
    callback attribute txDataCount;
    callback attribute txDataPollCount;
    callback attribute txBeaconCount;
    callback attribute txBeaconRequestCount;
    callback attribute txOtherCount;
    callback attribute txRetryCount;
    callback attribute txDirectMaxRetryExpiryCount;
    callback attribute txIndirectMaxRetryExpiryCount;
    callback attribute txErrCcaCount;
    callback attribute txErrAbortCount;
    callback attribute txErrBusyChannelCount;
    callback attribute rxTotalCount;
    callback attribute rxUnicastCount;
    callback attribute rxBroadcastCount;
    callback attribute rxDataCount;
    callback attribute rxDataPollCount;
    callback attribute rxBeaconCount;
    callback attribute rxBeaconRequestCount;
    callback attribute rxOtherCount;
    callback attribute rxAddressFilteredCount;
    callback attribute rxDestAddrFilteredCount;
    callback attribute rxDuplicatedCount;
    callback attribute rxErrNoFrameCount;
    callback attribute rxErrUnknownNeighborCount;
    callback attribute rxErrInvalidSrcAddrCount;
    callback attribute rxErrSecCount;
    callback attribute rxErrFcsCount;
    callback attribute rxErrOtherCount;
    callback attribute activeTimestamp;
    callback attribute pendingTimestamp;
    callback attribute delay;
    callback attribute securityPolicy;
    callback attribute channelPage0Mask;
    callback attribute operationalDatasetComponents;
    callback attribute activeNetworkFaultsList;
    callback attribute generatedCommandList;
    callback attribute acceptedCommandList;
    callback attribute attributeList;
    ram      attribute featureMap default = 0x000F;
    ram      attribute clusterRevision default = 1;
  }

  server cluster WiFiNetworkDiagnostics {
    callback attribute bssid;
    callback attribute securityType;
    callback attribute wiFiVersion;
    callback attribute channelNumber;
    callback attribute rssi;
    callback attribute beaconLostCount;
    callback attribute beaconRxCount;
    callback attribute packetMulticastRxCount;
    callback attribute packetMulticastTxCount;
    callback attribute packetUnicastRxCount;
    callback attribute packetUnicastTxCount;
    callback attribute currentMaxRate;
    callback attribute overrunCount;
    callback attribute generatedCommandList;
    callback attribute acceptedCommandList;
    callback attribute attributeList;
    ram      attribute featureMap default = 3;
    ram      attribute clusterRevision default = 0x0001;
  }

  server cluster AdministratorCommissioning {
    callback attribute windowStatus;
    callback attribute adminFabricIndex default = 1;
    callback attribute adminVendorId;
    callback attribute generatedCommandList;
    callback attribute acceptedCommandList;
    callback attribute attributeList;
    ram      attribute featureMap;
    ram      attribute clusterRevision default = 1;
  }

  server cluster OperationalCredentials {
    callback attribute NOCs;
    callback attribute fabrics;
    callback attribute supportedFabrics;
    callback attribute commissionedFabrics;
    callback attribute trustedRootCertificates;
    callback attribute currentFabricIndex;
    callback attribute generatedCommandList;
    callback attribute acceptedCommandList;
    callback attribute attributeList;
    ram      attribute featureMap;
    ram      attribute clusterRevision default = 1;
  }

  server cluster GroupKeyManagement {
    callback attribute groupKeyMap;
    callback attribute groupTable;
    callback attribute maxGroupsPerFabric;
    callback attribute maxGroupKeysPerFabric;
    callback attribute generatedCommandList;
    callback attribute acceptedCommandList;
    callback attribute attributeList;
    ram      attribute featureMap;
    ram      attribute clusterRevision default = 1;
  }
}


