ELF Header:
  Magic:   7f 45 4c 46 01 01 01 00 00 00 00 00 00 00 00 00 
  Class:                             ELF32
  Data:                              2's complement, little endian
  Version:                           1 (current)
  OS/ABI:                            UNIX - System V
  ABI Version:                       0
  Type:                              EXEC (Executable file)
  Machine:                           ARM
  Version:                           0x1
  Entry point address:               0x3199
  Start of program headers:          52 (bytes into file)
  Start of section headers:          1285596 (bytes into file)
  Flags:                             0x5000400, Version5 EABI, hard-float ABI
  Size of this header:               52 (bytes)
  Size of program headers:           32 (bytes)
  Number of program headers:         4
  Size of section headers:           40 (bytes)
  Number of section headers:         31
  Section header string table index: 30

Section Headers:
  [Nr] Name              Type            Addr     Off    Size   ES Flg Lk Inf Al
  [ 0]                   NULL            00000000 000000 000000 00      0   0  0
  [ 1] rom_start         PROGBITS        00000000 0000c0 000100 00 WAX  0   0  4
  [ 2] text              PROGBITS        00000100 0001c0 009b64 00  AX  0   0  4
  [ 3] .ARM.exidx        ARM_EXIDX       00009c64 009d24 000008 00  AL  2   0  4
  [ 4] initlevel         PROGBITS        00009c6c 009d2c 000070 00   A  0   0  4
  [ 5] devices           PROGBITS        00009cdc 009d9c 000090 00   A  0   0  4
  [ 6] sw_isr_table      PROGBITS        00009d6c 009e2c 000180 00  WA  0   0  4
  [ 7] log_const_section PROGBITS        00009eec 009fac 000040 00   A  0   0  4
  [ 8] log_backends_sect PROGBITS        00009f2c 009fec 000010 00   A  0   0  4
  [ 9] device_handles    PROGBITS        00009f3c 009ffc 000024 00   A  0   0  2
  [10] rodata            PROGBITS        00009f60 00a020 001038 00   A  0   0 16
  [11] .ramfunc          PROGBITS        20000000 00b240 000000 00   W  0   0  1
  [12] datas             PROGBITS        20000000 00b058 00014c 00  WA  0   0  4
  [13] device_states     PROGBITS        2000014c 00b1a4 000018 00  WA  0   0  4
  [14] k_mutex_area      PROGBITS        20000164 00b1bc 000064 00  WA  0   0  4
  [15] k_sem_area        PROGBITS        200001c8 00b220 000020 00  WA  0   0  4
  [16] bss               NOBITS          200001e8 00b268 001d30 00  WA  0   0  8
  [17] noinit            NOBITS          20001f80 00b268 003aa0 00  WA  0   0 128
  [18] .comment          PROGBITS        00000000 00b240 0000f8 01  MS  0   0  1
  [19] .debug_aranges    PROGBITS        00000000 00b338 001df8 00      0   0  8
  [20] .debug_info       PROGBITS        00000000 00d130 0980a1 00      0   0  1
  [21] .debug_abbrev     PROGBITS        00000000 0a51d1 012f98 00      0   0  1
  [22] .debug_line       PROGBITS        00000000 0b8169 02cedb 00      0   0  1
  [23] .debug_frame      PROGBITS        00000000 0e5044 0047d0 00      0   0  4
  [24] .debug_str        PROGBITS        00000000 0e9814 00ee18 01  MS  0   0  1
  [25] .debug_loc        PROGBITS        00000000 0f862c 027853 00      0   0  1
  [26] .debug_ranges     PROGBITS        00000000 11fe80 008f58 00      0   0  8
  [27] .ARM.attributes   ARM_ATTRIBUTES  00000000 128dd8 000039 00      0   0  1
  [28] .symtab           SYMTAB          00000000 128e14 0099a0 10     29 1435  4
  [29] .strtab           STRTAB          00000000 1327b4 0074d3 00      0   0  1
  [30] .shstrtab         STRTAB          00000000 139c87 000152 00      0   0  1
Key to Flags:
  W (write), A (alloc), X (execute), M (merge), S (strings), I (info),
  L (link order), O (extra OS processing required), G (group), T (TLS),
  C (compressed), x (unknown), o (OS specific), E (exclude),
  y (purecode), p (processor specific)

Program Headers:
  Type           Offset   VirtAddr   PhysAddr   FileSiz MemSiz  Flg Align
  EXIDX          0x009d24 0x00009c64 0x00009c64 0x00008 0x00008 R   0x4
  LOAD           0x0000c0 0x00000000 0x00000000 0x0af98 0x0af98 RWE 0x10
  LOAD           0x00b058 0x20000000 0x0000af98 0x001e8 0x001e8 RW  0x4
  LOAD           0x00b268 0x200001e8 0x200001e8 0x00000 0x05838 RW  0x80

 Section to Segment mapping:
  Segment Sections...
   00     .ARM.exidx 
   01     rom_start text .ARM.exidx initlevel devices sw_isr_table log_const_sections log_backends_sections device_handles rodata 
   02     datas device_states k_mutex_area k_sem_area 
   03     bss noinit 
