#

##

##

##

##

##

##

    µVision Build Log
    Tool Versions:
    IDE-Version: µVision V5.37.0.0
    Copyright (C) 2022 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: Roeltin Louw, BlackBox Industries, LIC=53CS8-MYVVV-5V61K-CLDHM-SR479-UPXGN

    Tool Versions:
    Toolchain:       MDK-ARM Community  Version: 5.37.0.0
    Toolchain Path:  C:\Keil_v5\ARM\ARM_Compiler_5.06u7\Bin
    C Compiler:      Armcc.exe V5.06 update 7 (build 960)
    Assembler:       Armasm.exe V5.06 update 7 (build 960)
    Linker/Locator:  ArmLink.exe V5.06 update 7 (build 960)
    Library Manager: ArmAr.exe V5.06 update 7 (build 960)
    Hex Converter:   FromElf.exe V5.06 update 7 (build 960)
    CPU DLL:
    Dialog DLL:
    Target DLL:      Segger\JL2CM3.dll V2.99.42.0
    Dialog DLL:      TCM.DLL V1.56.1.0

    Project:
    C:\BlackBox\GitKraken\US-Cruizers\nRF5_SDK_17.1.0_ddde560\examples\ble_peripheral\ble_app_uart\pca10100\s140\arm5_no_packs\ble_app_uart_pca10100_s140.uvprojx
    Project File Date:  08/04/2023

    Output:
    *** Using Compiler 'V5.06 update 7 (build 960)', folder: 'C:\Keil_v5\ARM\ARM_Compiler_5.06u7\Bin'
    Build target 'flash_s140_nrf52_7.2.0_softdevice'
    Before Build - User command #1: attrib +R ..\..\..\..\..\..\components\softdevice\s140\hex\\*
    compiling nrf_soc.c...
    C:\Users\roelt\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.44.1\Device\Include\nrf52833.h(147): error:  #5: cannot open source input file "core_cm4.h": No such file or directory
      #include "core_cm4.h"                           /*!< ARM Cortex-M4 processor and core peripherals                              */
    ..\..\..\..\..\..\components\drivers_nrf\nrf_soc_nosd\nrf_soc.c: 0 warnings, 1 error
    compiling nrf_libuarte_async.c...
    ..\..\..\..\..\..\components\libraries\libuarte\nrf_libuarte_async.h(43): error:  #5: cannot open source input file "sdk_errors.h": No such file or directory
      #include "sdk_errors.h"
    ..\..\..\..\..\..\components\libraries\libuarte\nrf_libuarte_async.c: 0 warnings, 1 error
    compiling nrfx_rtc.c...
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_rtc.c(41): error:  #5: cannot open source input file "nrfx.h": No such file or directory
      #include
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_rtc.c: 0 warnings, 1 error
    compiling nrfx_ppi.c...
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_ppi.c(41): error:  #5: cannot open source input file "nrfx.h": No such file or directory
      #include
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_ppi.c: 0 warnings, 1 error
    compiling nrfx_timer.c...
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_timer.c(41): error:  #5: cannot open source input file "nrfx.h": No such file or directory
      #include
    ..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx_timer.c: 0 warnings, 1 error
    compiling main.c...
    ..\..\..\main.c(57): error:  #5: cannot open source input file "nordic_common.h": No such file or directory
      #include "nordic_common.h"
    ..\..\..\main.c: 0 warnings, 1 error
    compiling nrf_nvic.c...
    C:\Users\roelt\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.44.1\Device\Include\nrf52833.h(147): error:  #5: cannot open source input file "core_cm4.h": No such file or directory
      #include "core_cm4.h"                           /*!< ARM Cortex-M4 processor and core peripherals                              */
    ..\..\..\..\..\..\components\drivers_nrf\nrf_soc_nosd\nrf_nvic.c: 0 warnings, 1 error
    compiling nrf_libuarte_drv.c...
    ..\..\..\..\..\..\components\libraries\libuarte\nrf_libuarte_drv.h(43): error:  #5: cannot open source input file "sdk_errors.h": No such file or directory
      #include "sdk_errors.h"
    ..\..\..\..\..\..\components\libraries\libuarte\nrf_libuarte_drv.c: 0 warnings, 1 error
    compiling nrf_queue.c...
    ..\..\..\..\..\..\components\libraries\queue\nrf_queue.c(40): error:  #5: cannot open source input file "sdk_common.h": No such file or directory
      #include "sdk_common.h"
    ..\..\..\..\..\..\components\libraries\queue\nrf_queue.c: 0 warnings, 1 error
    "..\..\..\..\..\..\components\softdevice\s140\hex\s140_nrf52_7.2.0_softdevice.hex" - 9 Error(s), 0 Warning(s).

    Software Packages used:

    Package Vendor: NordicSemiconductor
                    http://developer.nordicsemi.com/nRF5_SDK/pieces/nRF_DeviceFamilyPack/NordicSemiconductor.nRF_DeviceFamilyPack.8.44.1.pack
                    NordicSemiconductor.nRF_DeviceFamilyPack.8.44.1
                    Nordic Semiconductor nRF ARM devices Device Family Pack with BSD license.
       * Component: Startup Version: 8.44.1

    Collection of Component include folders:
      ./RTE/_flash_s140_nrf52_7.2.0_softdevice
      C:/Users/roelt/AppData/Local/Arm/Packs/NordicSemiconductor/nRF_DeviceFamilyPack/8.44.1/Device/Include

    Collection of Component Files used:

       * Component: ARM::CMSIS:CORE:5.6.0

       * Component: NordicSemiconductor::Device:Startup:8.44.1
          Source file:   Device/Source/arm/arm_startup_nrf52833.s
          Include file:  Device/Include/system_nrf52833.h
          Source file:   Device/Source/system_nrf52.c
          Include file:  Device/Include/system_nrf.h
    Target not created.
    Build Time Elapsed:  00:00:01