skrug@DESKTOP-KJBLMH9 MINGW64 /c/A/s4/tools/buildprog

$ python buildprog.py -p -c both -b debug -d both

+------------+----------+---------+--------------+---------------------+---------------------+

| snr | snr conn | device | only reboot | core app programmed | core net programmed |

+------------+----------+---------+--------------+---------------------+---------------------+

| 1050171701 | ←[32mTrue←[0m | headset | Not selected | Selected TBD | Selected TBD |

| 1050131916 | ←[32mTrue←[0m | gateway | Not selected | Selected TBD | Selected TBD |

| 10 | ←[33mFalse←[0m | headset | Not selected | Selected TBD | Selected TBD |

+------------+----------+---------+--------------+---------------------+---------------------+

Invoking build step

Net core uses precompiled hex

Run: west build C:\A\s4 -b nrf5340\_audio\_dk\_nrf5340\_cpuapp -d C:\A\s4\build\dev\_headset\build\_debug

[0/14] Performing build step for 'empty\_net\_core\_subimage'

[0/5] Performing build step for 'b0n\_subimage'

ninja: no work to do.

[1/10] Performing build step for 'mcuboot\_subimage'

ninja: no work to do.

[4/6] Generating ../../zephyr/net\_core\_app\_test\_update.hex

image.py: sign the payload

[6/6] Running post-build ble5-ctr signing step...

0x00000001

image.py: sign the payload

input hex name C:\ncs\v2.4.0\nrf\lib\bin\bt\_ll\_acs\_nrf53\bin\ble5-ctr-rpmsg\_shifted\_3349.hex

relative path

Run: west build C:\A\s4 -b nrf5340\_audio\_dk\_nrf5340\_cpuapp -d C:\A\s4\build\dev\_gateway\build\_debug

[0/14] Performing build step for 'empty\_net\_core\_subimage'

[0/5] Performing build step for 'b0n\_subimage'

ninja: no work to do.

[1/10] Performing build step for 'mcuboot\_subimage'

ninja: no work to do.

[4/6] Generating ../../zephyr/net\_core\_app\_test\_update.hex

image.py: sign the payload

[6/6] Running post-build ble5-ctr signing step...

0x00000001

image.py: sign the payload

input hex name C:\ncs\v2.4.0\nrf\lib\bin\bt\_ll\_acs\_nrf53\bin\ble5-ctr-rpmsg\_shifted\_3349.hex

relative path

Using NET hex: C:\lib\bin\bt\_ll\_acs\_nrf53\bin\ble5-ctr-rpmsg\_3349.hex for 1050171701 headset left

Using NET hex: C:\lib\bin\bt\_ll\_acs\_nrf53\bin\ble5-ctr-rpmsg\_3349.hex for 1050131916 gateway

Programming net core on: 1050171701 headset left

Programming net core on: 1050131916 gateway

ERROR: The operation attempted is unavailable due to readback protection in

ERROR: your device. Please use --recover to unlock the device.

NOTE: For additional output, try running again with logging enabled (--log).

NOTE: Any generated log error messages will be displayed.

ERROR: The operation attempted is unavailable due to readback protection in

ERROR: your device. Please use --recover to unlock the device.

NOTE: For additional output, try running again with logging enabled (--log).

NOTE: Any generated log error messages will be displayed.

build\_prog.py finished. Report:

+------------+----------+---------+--------------+---------------------+---------------------+

| snr | snr conn | device | only reboot | core app programmed | core net programmed |

+------------+----------+---------+--------------+---------------------+---------------------+

| 1050171701 | True | headset | Not selected | Selected TBD | Failed |

| 1050131916 | True | gateway | Not selected | Selected TBD | Failed |

| 10 | False | headset | Not selected | Not selected | Not selected |

+------------+----------+---------+--------------+---------------------+---------------------+